## Uses of Class
com.rscja.deviceapi.RFIDWithUHFUART

- Packages that use RFIDWithUHFUART
  Package | Description
  --- | ---
  com.rscja.deviceapi |

- - ### Uses of RFIDWithUHFUART in com.rscja.deviceapi

    Subclasses of RFIDWithUHFUART in com.rscja.deviceapi
    Modifier and Type | Class and Description
    --- | ---
    `class` | `RFIDWithUHFA4` UHF模块 A4操作类 UHF module operation type 第一步:通过`init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`stopInventory()`函数。 Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
    `class` | `RFIDWithUHFA8` UHF模块 A8操作类 UHF module operation type 第一步:通过`init(Context context)` 连接读写器。 Step 1: Connect to the usb of the reader via`init(Context context)` 第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`stopInventory()`函数。 Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
    `class` | `RFIDWithUHFAxBase`
    `class` | `RFIDWithUHFRLM`

    Methods in com.rscja.deviceapi that return RFIDWithUHFUART
    Modifier and Type | Method and Description
    --- | ---
    `static RFIDWithUHFUART` | RFIDWithUHFUART.`getInstance()` 获取UHF操作实例 Acquire UHF operation Instance