A B C D E F G H I K L M N O P R S T U V W Z

## W

WiegandData0 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
WiegandData1 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
WifiConfig - Class in com.rscja.deviceapi.entity
WifiConfig() - Constructor for class com.rscja.deviceapi.entity.WifiConfig
write(HF15693RequestEntity, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IHF15693
  写卡(Write card)
write(String, RFIDWithISO14443A.KeyType, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  写卡，此函数包括寻卡和密钥验证异常
  Card writing, this formula includes card searching and key verification err
write(int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  写卡，适用于Urltra light标签
  Card writing, used for Urltra light tag
write(int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  写卡
  card writing
write(int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  写卡
  card writing
write(String, RFIDWithISO14443A.KeyType, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  写卡，此函数包括寻卡和密钥验证异常
  Card writing, this formula includes card searching and key verification err
write(int, String) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  写卡，适用于Urltra light标签
  Card writing, used for Urltra light tag
write(int, String) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  写卡
  card writing
write(int, int, String) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  写卡
  card writing
writeAFI(HF15693RequestEntity, byte) - Method in interface com.rscja.deviceapi.interfaces.IHF15693
  写入AFI(Write AFi)
writeAFI(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  写入AFI
  Write AFi
writeAFI(int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  写入AFI
  Write AFi
writeBlock(byte, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  写卡(Write card)
writeData(String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
writeData(String, int, int, int, String, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
writeData(String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  向标签写入数据
  Write data in tag
writeData(String, int, int, int, String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  将数据写入指定标签
  Write data
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  将数据写入标签（write data to label）
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  将数据写入指定标签（write data to label）
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  将数据写入标签（write data to label）
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  将数据写入指定标签（write data to label）
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  将数据写入标签（write data to label）
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  将数据写入指定标签（write data to label）
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  将数据写入标签（write data to label）
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  将数据写入指定标签（write data to label）
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
writeData(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  向标签写入数据
  Write data in tag
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  将数据写入指定标签
  Write data
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
writeData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
writeData(String, int, int, int, String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
writeDataToEpc(String, int, int, int, String, String) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  将数据写入到EPC,而且自动适配盘点的EPC长度
  Write data to epc
writeDataToEpc(String, String) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  将数据写入到EPC,而且自动适配盘点的EPC长度
  Write data to epc
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  写标签到EPC (Write the label to the epc)
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  写标签到EPC (Write the label to the epc)
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  写标签到EPC (Write the label to the epc)
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  写标签到EPC (Write the label to the epc)
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  写标签到EPC (Write the label to the epc)
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  写标签到EPC (Write the label to the epc)
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  写标签到EPC (Write the label to the epc)
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  写标签到EPC (Write the label to the epc)
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
writeDataToEpc(String, int, int, int, String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
writeDataToEpc(String, String) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
writeDataWith4305Card(int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  写4305卡的某一页（0~31）数据
  write data in card 4305 at random page (0-31)
writeDataWith4305Card(int, String) - Method in class com.rscja.deviceapi.RFIDWithLF
  写4305卡的某一页（0~31）数据
  write data in card 4305 at random page (0-31)
writeDataWithHitagS(int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  写Hitag S卡中的某一页的数据
  Write data of random page in Hitag S card
writeDataWithHitagS(int, String) - Method in class com.rscja.deviceapi.RFIDWithLF
  写Hitag S卡中的某一页的数据
  Write data of random page in Hitag S card
writeDsfid(HF15693RequestEntity, byte) - Method in interface com.rscja.deviceapi.interfaces.IHF15693
  写入Dsfid(Write Dsfid)
writeDSFID(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  写入DSFID
  Write DSFID
writeDSFID(int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  写入DSFID
  Write DSFID
WriteFile(File, String, boolean) - Static method in class com.rscja.utility.FileUtility
WriteFile(File, byte[], boolean) - Static method in class com.rscja.utility.FileUtility

A B C D E F G H I K L M N O P R S T U V W Z