A B C D E F G H I K L M N O P R S T U V W Z

## P

P80_8953 - Static variable in class com.rscja.CWDeviceInfo
P80_8953_90 - Static variable in class com.rscja.CWDeviceInfo
parseBarcodeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析扫描条码返回的数据
parseBatteryData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析获取电量返回的数据
parseBeepData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析设置蜂鸣器返回的数据
parseBeepData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
  解析设置蜂鸣器返回的数据
parseBlinkOfLedData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBlockEraseDataData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBlockWriteData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBtDeleteAllTagToFlashData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBtGetAllTagNumFromFlashData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBtGetNewTagNumFromFlashData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseBtGetTagDataFromFlashData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseCloseLedData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseContinuousInventoryTagData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  循环盘点标签返回的数据
parseFastIdData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGBTagLockData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetAntData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetAntennaConnectStateReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetAntWorkTimeReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetCWData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetEPCTIDModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetFastIdData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetFrequencyModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetGen2Data(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetIOControlReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetPowerData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析获取功率返回的数据
parseGetProtocolData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析获取协议返回的数据
parseGetReaderAwaitSleepTimeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetReaderBeepStatusData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetReaderDestIpData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetReaderIpData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetRFLinkData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetTagfocusData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseGetTriggerWorkModeParaReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseGetWorkModeReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseInventorySingleTagData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析单次盘点标签返回的数据
parseKillData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析销毁标签返回的数据
parseLockData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析锁标签返回的数据
parseOpenLedData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseReadData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析读标签返回的数据
parseReadTagData_EPC(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析循环盘点标签返回的标签数据
parseReadTagData_EPC(byte[]) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
parseReadTagDataEPC_TID_USER(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseReadTagDataEPC_TID_USER(byte[]) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
parserUhfTagBuff_EPC_TID_USER(byte[], boolean) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
parseSetAntData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetAntWorkTimeReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetBeepTimeOfDuration(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetCWData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetEPCAndTIDModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetEPCAndTIDUserModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetEPCModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetFilterData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetFrequencyModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetGen2Data(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetIOControlReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetJumpFrequencyData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetPowerData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析设置功率返回的数据
parseSetProtocolData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析设置协议返回的数据
parseSetR6WorkModeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetReaderAwaitSleepTimeData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetReaderDestIpData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetReaderIpData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetRFLinkData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetSoftResetData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetTagfocusData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseSetTriggerWorkModeParaReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseSetWorkModeReceiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
parseStartInventoryTagData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析开始盘点标签返回的数据
parseSTM32VersionData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseStopInventoryData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析停止盘点标签返回的数据
parseTemperatureData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析模块温度返回的数据
parseUHFJump2BootData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseUHFStartUpdateData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseUHFStopUpdateData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseUHFUpdatingData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseVersionData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
parseWriteData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  解析写标签返回的数据
PLATFORM_MTK - Static variable in class com.rscja.CWDeviceInfo
PLATFORM_QCOM - Static variable in class com.rscja.CWDeviceInfo
powerOff(int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(int) - Method in class com.rscja.deviceapi.Module
  模块下电，仅下电不关串口
  module power off, power off only
powerOff(Context, int) - Method in class com.rscja.deviceapi.Module
  模块下电，仅下电不关串口
  module power off, power off only
powerOn(int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  模块上电，仅上电不开串口,通过DeviceAPI代码上电,配合`IModule.powerOff(int module)` 使用
  Module power on, power on only
powerOn(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  模块上电，仅上电不开串口,通过系统app上电,不经过DeviceAPI, 配合`IModule.powerOff(Context context,int module)` 使用
  Module power on, power on only
powerOn(int) - Method in class com.rscja.deviceapi.Module
  模块上电，仅上电不开串口,通过DeviceAPI代码上电,配合`Module.powerOff(int module)` 使用
  Module power on, power on only
powerOn(Context, int) - Method in class com.rscja.deviceapi.Module
  模块上电，仅上电不开串口,通过系统app上电,不经过DeviceAPI, 配合`Module.powerOff(Context context,int module)` 使用
  Module power on, power on only
print(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印字符
  print character
print(String) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印字符
  printe character
print(String, String) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印字符
  print character
print(Bitmap, int, int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印图片
  print pciture
print(Bitmap, int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印图片
  print picture
print(Bitmap) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印图片
  print picture
print(String, Printer.BarcodeType) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打印条码
  print barcode
print(byte[]) - Method in class com.rscja.deviceapi.Printer
  打印字符
  print character
print(String) - Method in class com.rscja.deviceapi.Printer
  打印字符
  printe character
print(String, String) - Method in class com.rscja.deviceapi.Printer
  打印字符
  print character
print(Bitmap, int, int) - Method in class com.rscja.deviceapi.Printer
  打印图片
  print pciture
print(Bitmap, int) - Method in class com.rscja.deviceapi.Printer
  打印图片
  print picture
print(Bitmap) - Method in class com.rscja.deviceapi.Printer
  打印图片
  print picture
print(String, Printer.BarcodeType) - Method in class com.rscja.deviceapi.Printer
  打印条码
  print barcode
Printer - Class in com.rscja.deviceapi
  打印机操作类
  Printer operation type
Printer.BarcodeType - Enum in com.rscja.deviceapi
  1D条码类型
Printer.PrinterStatus - Enum in com.rscja.deviceapi
Printer.PrinterStatusCallBack - Interface in com.rscja.deviceapi
PrinterBarcodeInvalidException - Exception in com.rscja.deviceapi.exception
PrinterBarcodeInvalidException(String) - Constructor for exception com.rscja.deviceapi.exception.PrinterBarcodeInvalidException
PrinterLowPager - Exception in com.rscja.deviceapi.exception
  打印机缺纸异常类
  printer lack paper exceotion type
PrinterLowPager() - Constructor for exception com.rscja.deviceapi.exception.PrinterLowPager
progress(int) - Method in interface com.rscja.deviceapi.FingerprintWithFIPS.GRABCallBack
  当前获取指纹图像的进度值
  current progress value of acquired fingerprint
progress(int) - Method in interface com.rscja.deviceapi.FingerprintWithTLK1NC.IUPImageCallback
  当前获取指纹图像的进度值
  current progress value of acquired fingerprint
progress(int) - Method in interface com.rscja.deviceapi.interfaces.IUpgradeProgress
PSAM - Class in com.rscja.deviceapi
  PSAM操作类
  PSAM operation type
PSAMException - Exception in com.rscja.deviceapi.exception
  PSAM异常
  PSAM exceprion
PSAMException(String) - Constructor for exception com.rscja.deviceapi.exception.PSAMException
ptCapture() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取指纹模版
  Acquire fingerprint template
ptCapture() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  获取指纹模版
  Acquire fingerprint template
ptConvertTemplateEx(FingerprintWithFIPS.DataFormat, byte[], int) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
ptConvertTemplateEx(FingerprintWithFIPS.DataFormat, byte[], int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS

A B C D E F G H I K L M N O P R S T U V W Z