A B C D E F G H I K L M N O P R S T U V W Z

## G

GBTagLockSendData(String, char, int, int, String, char, char, char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
Gen2Entity - Class in com.rscja.deviceapi.entity
Gen2Entity() - Constructor for class com.rscja.deviceapi.entity.Gen2Entity
genChar(Fingerprint.BufferEnum) - Method in class com.rscja.deviceapi.Fingerprint
  生成特征值（存于指定缓存区）
  Generate feature value( save in specified buffer zone)
genChar(Fingerprint.BufferEnum) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  生成特征值（存于指定缓存区）
  Generate feature value( save in specified buffer zone)
generate(FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  生成模版
generate(FingerprintWithZAZ.BufferEnum, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  生成模版
generateImg(byte[], String) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  生成bmp图片
  Generate bmp
generateImg(byte[], String) - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
generateImg(byte[], String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  生成bmp图片
  Generate bmp
generateImg(byte[], String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
generateLockCode(ArrayList<Integer>, int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取锁定码
  Get lock code
generateLockCode(ArrayList<Integer>, int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取锁标签的锁定码
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取锁定码(Get lock code)
  示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode);
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取锁定码(Get lock code)
  示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode);
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取锁定码(Get lock code)
  示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode);
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取锁定码(Get lock code)
  示例代码:比如锁定EPC区和USER区 (Sample code: such as locking EPC area and USER area) List lockBank=new ArrayList<>(); lockBank.add(IUHF.LockBank_EPC); lockBank.add(IUHF.LockBank_USER); int lockMode =IUHF.LockMode_LOCK; String hexLockCode=generateLockCode(lockBank,lockMode);
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取锁定码
  Get lock code
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
generateLockCode(ArrayList<Integer>, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
generateLockCode(ArrayList<Integer>, int) - Static method in class com.rscja.deviceapi.UHFProtocolParseBase
genericFunction(char, char[], char) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
genericFunction(char, char[], char) - Method in class com.rscja.deviceapi.RFIDWithISO15693
genericFunction_ex(char, char, char[], int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
genericFunction_ex(char, char, char[], int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
getAfi() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity
getAFI() - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  获取AFI值
  acquire AFI value
getAimId() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
getAllTagTotalFromFlash() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
  获取R2、R6 缓存的标签数量
  Acquire tag amounts in buffer of R2 and R6.
getAllTagTotalFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getAllTagTotalFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getAndroidDeviceHardwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getAndroidDeviceHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取android设备的硬件版本
getAndroidDeviceHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取android设备的硬件版本
getAndroidDeviceHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取android设备的硬件版本
getAndroidDeviceHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取android设备的硬件版本
getAnimalFlag() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的AnimalFlag
  acquire AnimalFlag of animal tag
getAnt() - Method in class com.rscja.deviceapi.entity.AntennaPowerEntity
getAnt() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getANT() - Method in interface com.rscja.deviceapi.interfaces.IMultipleAntenna
  获取当前设置的天线
getANT() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取天线
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取天线启用状态(Get the antenna enable status)
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取天线启用状态(Get the antenna enable status)
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取天线启用状态(Get the antenna enable status)
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取天线启用状态(Get the antenna enable status)
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
  获取当前设置的天线
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取天线
getANT() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getAntennaConnectState() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
getAntennaConnectState() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getAntennaConnectState() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
getAntennaConnectState() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getAntennaConnectStateSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getAntennaName() - Method in class com.rscja.deviceapi.entity.AntennaConnectState
getAntennaName() - Method in class com.rscja.deviceapi.entity.AntennaState
getAntennaPower() - Method in interface com.rscja.deviceapi.interfaces.IMultipleAntenna
  获取单个天线的功率
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取天线功率
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取天线功率
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取天线功率
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取天线功率
getAntennaPower() - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
getAntennaWorkTime(AntennaEnum) - Method in interface com.rscja.deviceapi.interfaces.IMultipleAntenna
  获取天线工作时间
getAntennaWorkTime(AntennaEnum) - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取天线工作时间
getAntennaWorkTime(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取天线工作时间(Get the working time of the antenna)
getAntennaWorkTime(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取天线工作时间(Get the working time of the antenna)
getAntennaWorkTime(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取天线工作时间(Get the working time of the antenna)
getAntennaWorkTime(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取天线工作时间(Get the working time of the antenna)
getAntennaWorkTime(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFAxBase
getAntennaWorkTime(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getAntennaWorkTime(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取天线工作时间
getAntennaWorkTime(AntennaEnum) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getAntSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getAntWorkTimeSendData(byte) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getAppWhiteList() - Method in interface com.rscja.system.ISystemInterfaces
  获取App白名单列表
getBalance() - Method in class com.rscja.deviceapi.CardWithBYL
  获取余额和有效期
getBalance() - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  获取余额和有效期
getBarcodeBytesData() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  条码原始数据
getBarcodeData() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  条码数据
getBarcodeDecoder() - Method in class com.rscja.barcode.BarcodeFactory
getBarcodeName(int) - Method in class com.rscja.barcode.BarcodeSymbolUtility
  获取条码名称(get barcode name)
getBarcodeName() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  条码类型
getBarcodeName(int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeSymbolUtility
getBarcodeSymbology() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  symbologyCode 条码类型code
getBattery() - Method in class com.rscja.deviceapi.BluetoothReader
getBattery() - Method in interface com.rscja.deviceapi.interfaces.IReader
  获取电池电量
  Acquire battery capacity
getBattery() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getBatterySendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取电量的发送数据
getBeepSendData(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取设置蜂鸣器的发送数据
getBeepSendData(boolean) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
  获取设置蜂鸣器的发送数据
getBleHardwareVersion() - Method in class com.rscja.deviceapi.BluetoothReader
getBleHardwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
getBluetoothVersion() - Method in class com.rscja.deviceapi.BluetoothReader
getBluetoothVersion() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  获取蓝牙版本号(acquire Bluetooth version)
getBrokenId(int, int, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
getBrokenId(int, int, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
getBytes(char[]) - Static method in class com.rscja.utility.StringUtility
  char类型数组转byte类型数组
getChars(byte[]) - Static method in class com.rscja.utility.StringUtility
  byte类型数组转char类型数组
getConnectionStatus() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
getConnectStatus() - Method in class com.rscja.deviceapi.BluetoothReader
getConnectStatus() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  获取蓝牙连接状态(Acquire Bluetooth connection status)
getConnectStatus() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取UHF连接状态
  Acquire UHF connection status
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取连接状态(Acquire UHF connection status)
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取连接状态(Acquire UHF connection status)
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取连接状态(Acquire UHF connection status)
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取连接状态(Acquire UHF connection status)
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取UHF连接状态
  Acquire UHF connection status
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getConnectStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getControlWork() - Method in class com.rscja.deviceapi.entity.GPIOInfo
getCount() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getCountryID() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的国家代码
  acquire national code of animal tag
getCpuType() - Method in class com.rscja.CWDeviceInfo
getCW() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取连续波设置
  Acquire CW setup
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取连续波状态(Get CW status)
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取连续波状态(Get CW status)
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取连续波状态(Get CW status)
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取连续波状态(Get CW status)
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取连续波设置
  Acquire CW setup
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getCW() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getCWSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getData() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取数据，仅对数据文件类型有效
  acquire data, it is only valid for data file type only
getData() - Method in class com.rscja.deviceapi.entity.GPIOInfo
getData() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签数据
  acquire tag data
getDataBlock() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的DataBlock
  acquire DataBlock of animal tag
getDecoderSVersionInfo() - Method in class com.rscja.barcode.BarcodeDecoder
  返回扫描头和解码库信息
getDecodeTime() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  解码时间
getDesfid() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity
getDESFID() - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  获取DESFID值
  acquire DESFID value
getDestIP() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取目标IP
getDestIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getDestIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取目标IP
getDestIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getDeviceInfo() - Static method in class com.rscja.CWDeviceInfo
getDeviceInfo() - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  获取模块的设备信息
getDeviceInfo() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  获取模块的设备信息
getDevices(BluetoothDevice, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.ScanBTCallback
getDeviceVersion() - Method in class com.rscja.deviceapi.FingerprintSM206B
  获取指纹模块固件版本
getDeviceVersion() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintSM206B
getDns1() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getDns2() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getEmptyId(int, int) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  获取指定编号范围内可注册的首个编号
getEmptyId(int, int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  获取指定编号范围内可注册的首个编号
getEncryptionType() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取加密方式
  acquire encryption method
getEngineExtrasInfo() - Method in class com.rscja.barcode.Barcode2DSHardwareInfo
  扫描头额外的扩展信息
getEngineExtrasInfo() - Method in interface com.rscja.barcode.IBarcode2DSHardwareInfo
getEngineName() - Method in class com.rscja.barcode.Barcode2DSHardwareInfo
  扫描头型号
getEngineName() - Method in interface com.rscja.barcode.IBarcode2DSHardwareInfo
getEnrollCount(int, int, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
getEnrollCount(int, int, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
getEPC() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getEPCAndTIDUserMode() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取当前循环盘点的模式(EPC或者EPC+TID或者EPC+TID+USER)
  Acquire current scan mode(EPC or EPC+TID or EPC+TID+USER)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取当前设置的盘点模式 (Get the currently set inventory mode)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取当前设置的盘点模式 (Get the currently set inventory mode)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取当前设置的盘点模式 (Get the currently set inventory mode)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取当前设置的盘点模式 (Get the currently set inventory mode)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  设置R6工作模式
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取当前循环盘点的模式(EPC或者EPC+TID或者EPC+TID+USER)
  Acquire current scan mode(EPC or EPC+TID or EPC+TID+USER)
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getEPCAndTIDUserMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getEpcBytes() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getEPCTIDModeSendData(char, char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getErrCode() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
getErrCode() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUSB
getErrCode() - Method in interface com.rscja.deviceapi.interfaces.IUHFOfAndroidUart
getErrCode() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
  获取`RFIDWithUHFUrxUsbToUart.init(UsbDevice, Context)`失败的错误码
  Acquire `RFIDWithUHFUrxUsbToUart.init(UsbDevice, Context)` error codes of failure.
getErrCode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  获取`RFIDWithUHFUSB.init(UsbDevice, Context)`失败的错误码
  Acquire `RFIDWithUHFUSB.init(UsbDevice, Context)` error codes of failure.
getErrorMsg(int) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
getEthernetIpConfig() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getEthernetIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取以太网配置信息
getEthernetIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取以太网配置信息
getEthernetIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取以太网配置信息
getEthernetIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取以太网配置信息
getExtraData(String) - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getFastIDSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getFileNo() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取文件号
  acquire file number
getFileSize() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取文件大小，仅对数据文件类型有效
  acquire file size, it is valid for data file type only
getFileType() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取文件类型
  acquire file type
getFingersCount() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取模块中采集的指纹数量
  Acquire collected fingerprint amounts in module.
getFingersCount() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  获取模块中采集的指纹数量
  Acquire collected fingerprint amounts in module.
getFingerTemplate() - Method in class com.rscja.deviceapi.FingerprintSM206B
  获取指纹模板数据，用户录入 1 次指纹，生成 256 字节指纹特征值
getFingerTemplate() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintSM206B
getFrequencyMode() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
getFrequencyMode() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  读取模块的工作模式
  Read work mode of module
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取模块的工作频率(Get the working frequency of the module)
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取模块的工作频率(Get the working frequency of the module)
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取模块的工作频率(Get the working frequency of the module)
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取模块的工作频率(Get the working frequency of the module)
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  读取模块的工作模式
  Read work mode of module
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getFrequencyMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getFrequencyModeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getFullData() - Method in class com.rscja.deviceapi.entity.GPIOInfo
getGateway() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getGen2() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取Gen2参数
  Acquire Gen2 parameter
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取GEN2参数值(Get GEN2 parameter value)
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取Gen2参数
  Acquire Gen2 parameter
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getGen2() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getGen2SendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getGpiName() - Method in class com.rscja.deviceapi.entity.GPIStateEntity
getGpiState() - Method in class com.rscja.deviceapi.entity.GPIStateEntity
getGpoName() - Method in class com.rscja.deviceapi.entity.GPOEntity
getGpoState() - Method in class com.rscja.deviceapi.entity.GPOEntity
getHardwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读取硬件版本
  read hardware version
getHardwareVersion() - Method in interface com.rscja.deviceapi.interfaces.IUHFOfAndroidUart
getHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithLF
  读取硬件版本
  read hardware version
getHardwareVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getHF14443A() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取14443A操作对象 (Get the 14443A operation object)
getHF14443B() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取14443B操作对象 (Get the 14443B operation object)
getHF15693() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取15693操作对象 (Get the 15693 operation object)
getHFVersion() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取高频版本号(Get the HF version)
getId() - Method in class com.rscja.deviceapi.entity.HF14443RequestEntity
getId() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签ID
  acquire tag ID
getId() - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
  获取指纹模块ID(十六进制)
  Acquire fingerprint module ID (hex)
getID() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取指纹ID
  Acquire fingerprint ID
getID() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  获取指纹ID
  Acquire fingerprint ID
getIDAndPowerWithWattmeter() - Method in class com.rscja.deviceapi.Infrared
  获取电表ID和电能值,97标准
  Acquire powermeter ID and energy value, 97 standard
getIDAndPowerWithWattmeter(int) - Method in class com.rscja.deviceapi.Infrared
  获取电表ID和电能值
  Acquire powermeter ID and energy value
getIDAndPowerWithWattmeter() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  获取电表ID和电能值,97标准
  Acquire powermeter ID and energy value, 97 standard
getIDAndPowerWithWattmeter(int) - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  获取电表ID和电能值
  Acquire powermeter ID and energy value
getIdBytes() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签ID
  acquire tag ID
getIdData() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取64bit的识别号数据，十六进制表示
  acquire 64bit identification number, hexdecimal
getImage() - Method in class com.rscja.deviceapi.Fingerprint
  获取指纹图像（存于模块图像缓存区）
  Acquire fingerprint image( save in buffer zone of module image)
getImage() - Method in class com.rscja.deviceapi.FingerprintSM206B
getImage(int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  从采集器采集指纹图像并保存于 ImageBuffer 中
getImage() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取指纹图像（存于模块图像缓存区）
  Acquire fingerprint image( save in buffer zone of module image)
getImage() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintSM206B
getImage(int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  从采集器采集指纹图像并保存于 ImageBuffer 中
getIndex() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getInputStatus() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取输入口状态
getInputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getInputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取输入口状态
getInputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getInstance() - Static method in class com.rscja.barcode.Barcode2DSHardwareInfo
getInstance() - Static method in class com.rscja.barcode.BarcodeFactory
getInstance() - Static method in class com.rscja.barcode.BarcodeSymbolUtility
getInstance() - Static method in class com.rscja.barcode.BarcodeUtility
  获取条码操作实例 Acquire barcode operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.Barcode1D
  获取一维条码操作实例
  Acquire 1D barcode operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.Barcode2D
  获取二维条码操作实例
  * Acquire 2D barcode operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.BluetoothReader
  Get BluetoothReader
getInstance() - Static method in class com.rscja.deviceapi.CardWithBYL
  获取RFID低频操作实例
getInstance() - Static method in class com.rscja.deviceapi.Fingerprint
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance.
getInstance() - Static method in class com.rscja.deviceapi.FingerprintSM206B
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取指纹模块操作实例
  Acquire fingerprint module operation Instance
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithMorpho
  获取指纹模块操作实例
  acquire fingerprint module operation eample
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithTLK1NC
getInstance() - Static method in class com.rscja.deviceapi.FingerprintWithZAZ
  获取指纹模块操作实例
  acquire fingerprint module operation eample
getInstance() - Static method in class com.rscja.deviceapi.Infrared
getInstance() - Static method in class com.rscja.deviceapi.LedLight
  获取LED灯操作实例
  Acquire LED operation example
getInstance() - Static method in class com.rscja.deviceapi.Module
  获取操作实例
  Acquire operation Instance
getInstance() - Static method in class com.rscja.deviceapi.Printer
  获取打印机模块操作实例
  Acquire printer module operation Instance
getInstance() - Static method in class com.rscja.deviceapi.PSAM
  获取PSAM操作实例
  Acquire PSAM operation Instance
getInstance() - Static method in class com.rscja.deviceapi.R1HFAndPsamManage
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO14443A
  获取ISO14443A协议操作实例
  Acquire ISO14443A protocol operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  获取ISO14443A CPU卡协议操作实例
  Acquire ISO14443A CPU card protocol operation example
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO14443B
  获取ISO14443B协议操作实例
  Acquire ISO14443B protocol operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithISO15693
  获取ISO15693协议操作实例
  Acquire ISO15693 protocol operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithLF
  获取RFID低频操作实例
  Acquire RFID LF operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFA4
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFA8
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFBLE
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFRLM
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFUART
  获取UHF操作实例
  Acquire UHF operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取UHF操作实例
  Acquire UHF operation Instance
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getInstance() - Static method in class com.rscja.deviceapi.RFIDWithUHFUSB
getInstance() - Static method in class com.rscja.deviceapi.ScanerLedLight
  获取LED灯操作实例
  Acquire LED light operation example
getInstance() - Static method in class com.rscja.deviceapi.UsbFingerprint
getInstance() - Static method in class com.rscja.scanner.led.ScanLedManage
getInstance() - Static method in class com.rscja.system.SystemInterfacesFactory
getIntegerSomeBit(int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  取整数的某一位
  get one place of integer
getIntegerSomeBit(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  取整数的某一位
  get one place of integer
getInventorySingleTagSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取开启单次盘点标签的发送数据
getIOControlSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getIp() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIpv6Dns1() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIpv6Dns2() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIpv6Ip1() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIpv6Ip2() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getIpv6Ip3() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getKillSendData(String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取销毁标签的发送数据
getLastDecImage(BarcodeDecoder.IBarcodeImageCallback) - Method in class com.rscja.barcode.BarcodeDecoder
getLastDecImage(BarcodeDecoder.IBarcodeImageCallback) - Method in interface com.rscja.deviceapi.interfaces.IZebra2DSoftDecoder
getLastDecImage(Context) - Method in interface com.rscja.scanner.IScanner
getLastDecImage(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
getLinkFrequency() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  Link Frequency 设置(Link Frequency setting)
getLocationValue(int) - Method in interface com.rscja.deviceapi.interfaces.IUHFLocationCallback
getLockSendData(String, int, int, int, String, String) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取锁标签需要发送的数据
getMainboardVersion() - Method in interface com.rscja.deviceapi.interfaces.IBluetoothData
  获取主板版本
getManufactor() - Method in class com.rscja.barcode.Barcode2DSHardwareInfo
  扫描头厂家
getManufactor() - Method in interface com.rscja.barcode.IBarcode2DSHardwareInfo
getMaxQ() - Method in class com.rscja.deviceapi.entity.Gen2Entity
getMaxValue() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取最大值，仅对值文件类型有效
  acquire maximum value, it is valid for value file type only
getMessage(int) - Method in class com.rscja.deviceapi.CardWithBYL
  将错误代码转换为语义消息
getMessage(int) - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  将错误代码转换为语义消息
getMinQ() - Method in class com.rscja.deviceapi.entity.Gen2Entity
getMinValue() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取最小值，仅对值文件类型有效
  acquire minimum value, it is valid for value file type only
getMode() - Method in class com.rscja.deviceapi.entity.InventoryModeEntity
  获取盘点模式(Get inventory mode)
getModel() - Method in class com.rscja.CWDeviceInfo
getModelAndCpu() - Method in class com.rscja.CWDeviceInfo
getMorphoDescriptor() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
getMorphoDescriptor() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
getMorphoPIDSN() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  获取指纹版本
  acquire fingerprint version
getMorphoPIDSN() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  获取指纹版本
  acquire fingerprint version
getMorphoSecurityLevel() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
getMorphoSecurityLevel() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
getNationalID() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的NationalID信息
  acquire national infor of animal tag
getNetworkClass(Activity) - Static method in class com.rscja.utility.NetUtils
getNetworkType() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getNetworkType(Activity) - Static method in class com.rscja.utility.NetUtils
  获取当前网络类型
getNewTagTotalFromFlash() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
getNewTagTotalFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getNewTagTotalFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getNumParameter(int) - Method in interface com.rscja.deviceapi.interfaces.IZebra2DSoftDecoder
getOriginalUID() - Method in class com.rscja.deviceapi.entity.ISO15693Entity
  获取标签原始的UID
  acquire original UID of tag
getParam(int) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  根据指定的参数类型，读取设备参数
getParam(int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  根据指定的参数类型，读取设备参数
getPassword() - Method in class com.rscja.deviceapi.entity.WifiConfig
getPc() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getPlatform() - Method in class com.rscja.CWDeviceInfo
getPointDouble(int, double) - Static method in class com.rscja.utility.NumberTool
  保留指定位数小数的double值
getPointDouble(int, int) - Static method in class com.rscja.utility.NumberTool
  保留指定位数小数的double值
getPointDouble(int, long) - Static method in class com.rscja.utility.NumberTool
  保留指定位数小数的double值
getPointDouble(int, String) - Static method in class com.rscja.utility.NumberTool
  保留指定位数小数的double值
getPointFloat(int, float) - Static method in class com.rscja.utility.NumberTool
getPort() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getPower() - Method in class com.rscja.deviceapi.entity.AntennaPowerEntity
getPower() - Method in interface com.rscja.deviceapi.interfaces.ISingleAntenna
  读取模块的功率
  Read module output power
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  读取模块的功率
  Read module output power
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getPower() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getPowerSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取功率的发送数据
getPrefix() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  前缀
getPrintCodePage() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
getPrintCodePage() - Method in class com.rscja.deviceapi.Printer
getPrinterType() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
getPrinterType() - Method in class com.rscja.deviceapi.Printer
getProtocol() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取协议
  Acquire protocol
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取协议(Get the protocol)
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取协议(Get the protocol)
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取协议(Get the protocol)
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取协议(Get the protocol)
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取协议
  Acquire protocol
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getProtocol() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getProtocolSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取协议需要发送数据
getProxy() - Method in class com.rscja.deviceapi.entity.WifiConfig
getPSAM() - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  获取PSAM操作对象 (Get the PSAM operation object)
getPsamCardID() - Method in class com.rscja.deviceapi.CardWithBYL
  获取psam卡id
getPsamCardID() - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  获取psam卡id
getPTInfo() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  获取模块信息
  Acquire module information
getPTInfo() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  获取模块信息
  Acquire module information
getPwm() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取占空比，仅适用于R2000模块
  acquire duty ratio, used for R2000 module only
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取占空比 (Get the duty cycle)
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取占空比 (Get the duty cycle)
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取占空比 (Get the duty cycle)
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取占空比 (Get the duty cycle)
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取占空比，仅适用于R2000模块
  acquire duty ratio, used for R2000 module only
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getPwm() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getQ() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取Q值(Q value)
getQueryDR() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的DR参数(DR parameter of the query command)
getQueryM() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的M参数(M parameter of the query command )
getQuerySel() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的sel参数(sel parameter of the query command)
getQuerySession() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的session参数(session parameter of the query command)
getQueryTarget() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的Target参数(Target parameter of the query command)
getQueryTRext() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取query命令的TRext参数(TRext parameter of the query command )
getRandomData() - Method in class com.rscja.deviceapi.Fingerprint
  获取随机数，检测模块是否正常
  Acquire random number, detect module is normal or not.
getRandomData() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取随机数，检测模块是否正常
  Acquire random number, detect module is normal or not.
getRawData() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取原始数据，十六进制表示
  acquire original data, hexdecimal
getReaderAwaitSleepTime() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
  获取读写器等待休眠的时间
getReaderAwaitSleepTime() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getReaderAwaitSleepTime() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getReaderAwaitSleepTimeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getReaderBeepStatusSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getReaderCurrentIp() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getReaderCurrentIp() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取设备当前的IP地址
getReaderCurrentIp() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取设备当前的IP地址
getReaderCurrentIp() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取设备当前的IP地址
getReaderCurrentIp() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取设备当前的IP地址
getReaderDestIpSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getReaderIpSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getReadPermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取读取权限
  acquire read authorization
getReadSendData(String, int, int, int, String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取读标签的发送数据
getReadTagSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取在循环盘点标签的模式中,读取缓存标签的发送数据
getReadWritePermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取读写权限
  acquire read-write authorization
getRemain() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getReserved() - Method in class com.rscja.deviceapi.entity.AnimalEntity
  获取动物标签的Reserved信息
  acquire Reserved infor of animal tag
getReserved() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getResultCode() - Method in class com.rscja.deviceapi.entity.BarcodeEntity
  结果码 `BarcodeDecoder.DECODE_SUCCESS`
  `BarcodeDecoder.DECODE_FAILURE`
  `BarcodeDecoder.DECODE_TIMEOUT`
  `BarcodeDecoder.DECODE_CANCEL`
getRFLink() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取链路参数
  acquire link parameter
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取链路参数(Get link parameters)
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取链路参数(Get link parameters)
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取链路参数(Get link parameters)
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取链路参数(Get link parameters)
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取链路参数
  acquire link parameter
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getRFLink() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getRFLinkSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getRssi() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getScanBarcodeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取扫描条码的发送数据
getScanLed() - Method in class com.rscja.scanner.led.ScanLedManage
getScannerInerface() - Static method in class com.rscja.scanner.utility.ScannerUtility
getScannerParameter(Context) - Method in interface com.rscja.scanner.IScanner
getScannerParameter(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
getSecurityType() - Method in class com.rscja.deviceapi.entity.WifiConfig
getSelectAction() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取select 命令的Action参数 (Action parameter of the select command)
getSelectTarget() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取select命令的Target参数 (Target parameter of the select command)
getSelectTruncate() - Method in class com.rscja.deviceapi.entity.Gen2Entity
  获取select命令的Truncate参数(Truncate parameter of the select command)
getSetSoftResetSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getSN() - Method in interface com.rscja.system.ISystemInterfaces
  获取SN号
getSsid() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getSsid() - Method in class com.rscja.deviceapi.entity.WifiConfig
getStartInventoryTagSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取循环盘点标签的发送数据
getStartQ() - Method in class com.rscja.deviceapi.entity.Gen2Entity
getStaticIpConfig() - Method in class com.rscja.deviceapi.entity.WifiConfig
getStatus(ConnectionStatus, T) - Method in interface com.rscja.deviceapi.interfaces.ConnectionStatusCallback
getStatusMsg(int) - Static method in class com.rscja.deviceapi.FingerprintWithFIPS
getStatusMsg(int) - Static method in class com.rscja.deviceapi.FingerprintWithMorpho
getStatusMsg(int) - Static method in class com.rscja.deviceapi.FingerprintWithTLK1NC
getSTM32Version() - Method in class com.rscja.deviceapi.BluetoothReader
getSTM32Version() - Method in interface com.rscja.deviceapi.interfaces.IReader
  获取stm32版本号(Acquire stm32 version )
getSTM32Version() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
getSTM32Version() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getSTM32Version() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
getSTM32Version() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getSTM32Version() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getSTM32VersionSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getStopInventorySendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取停止循环盘点标签的发送数据
getStrParameter(int) - Method in interface com.rscja.deviceapi.interfaces.IZebra2DSoftDecoder
getStrProperty(int) - Method in interface com.rscja.deviceapi.interfaces.IZebra2DSoftDecoder
getSubnetMask() - Method in class com.rscja.deviceapi.entity.ReaderIPEntity
getSystemInterfaces(Context) - Method in class com.rscja.system.SystemInterfacesFactory
getTagDataFromFlash() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
  获取R2、R6缓存的标签信息
  Acquire tag information in buffer of R2 and R6
getTagDataFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getTagDataFromFlash() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getTagfocusSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getTcpServiceVersion() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getTcpServiceVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取UHF TCP服务版本
getTcpServiceVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取UHF TCP服务版本
getTcpServiceVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取UHF TCP服务版本
getTcpServiceVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取UHF TCP服务版本
getTeam() - Method in class com.rscja.CWDeviceInfo
getTemperature() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取模块温度
  Acquire module Temperature
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取UHF模块温度 (Get UHF module temperature)
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取UHF模块温度 (Get UHF module temperature)
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取UHF模块温度 (Get UHF module temperature)
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取UHF模块温度 (Get UHF module temperature)
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取模块温度
  Acquire module Temperature
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getTemperature() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getTemperatureSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取模块温度
getTid() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getTriggerWorkModePara() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取触发工作模式参数
getTriggerWorkModePara() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getTriggerWorkModePara() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取触发工作模式参数
getTriggerWorkModePara() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getTriggerWorkModeParaSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getType() - Method in class com.rscja.deviceapi.entity.HF14443RequestEntity
getType() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity
getType() - Method in class com.rscja.deviceapi.entity.SimpleRFIDEntity
  获取标签类型
  acquire tag type
getUhfReaderIP() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取UHF读写器IP
getUhfReaderIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getUhfReaderIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取UHF读写器IP
getUhfReaderIP() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getUhfvalidData(AbstractQueue<Byte>, int, boolean) - Method in class com.rscja.deviceapi.UHFProtocolParseBase
getUid() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity
getUID() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUID() - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUIDBytes() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUIDBytes() - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  获取卡片ID
  Acquire card ID
getUidTypeB() - Method in interface com.rscja.deviceapi.interfaces.IHF14443B
  获取卡片ID (Acquire card ID)
getUIDWith4450Card() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  获取UID,用于4450Card
  Acquire UID, used for 4450 card
getUIDWith4450Card() - Method in class com.rscja.deviceapi.RFIDWithLF
  获取UID,用于4450Card
  Acquire UID, used for 4450 card
getUIDWithHID() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读取HID卡
  Read HID card
getUIDWithHID() - Method in class com.rscja.deviceapi.RFIDWithLF
  读取HID卡
  Read HID card
getUIDWithHitagS() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  获取UID,用于hitag S
  Acquire UID, used for hitag S
getUIDWithHitagS() - Method in class com.rscja.deviceapi.RFIDWithLF
  获取UID,用于hitag S
  Acquire UID, used for hitag S
getUpdatePermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取修改权限
  acquire modify authorization
getUsbDeviceList(Context) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUSB
getUsbDeviceList(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  获取usb列表
getUser() - Method in class com.rscja.deviceapi.entity.UHFTAGInfo
getUserLength() - Method in class com.rscja.deviceapi.entity.InventoryModeEntity
  获取要盘点的User区长度(User area data length)
getUserOffset() - Method in class com.rscja.deviceapi.entity.InventoryModeEntity
  获取要盘点的User区起始地址(User area start address)
getValue() - Method in enum com.rscja.barcode.BarcodeUtility.ModuleType
getValue() - Method in enum com.rscja.deviceapi.entity.HF15693RequestEntity.TagType
getValue() - Method in enum com.rscja.deviceapi.enums.AntennaEnum
getValue(int) - Static method in enum com.rscja.deviceapi.enums.AntennaEnum
getValue() - Method in enum com.rscja.deviceapi.Fingerprint.BufferEnum
  获取枚举的值
  Acquire example value
getValue() - Method in enum com.rscja.deviceapi.FingerprintWithTLK1NC.BufferEnum
  获取枚举的值
  Acquire example value
getValue() - Method in enum com.rscja.deviceapi.FingerprintWithZAZ.BufferEnum
  获取枚举的值
  Acquire example value
getValue() - Method in enum com.rscja.deviceapi.RFIDWithISO14443A.DESFireEncryptionTypekEnum
getValue() - Method in enum com.rscja.deviceapi.RFIDWithISO14443A.DESFireFileTypekEnum
getValue() - Method in enum com.rscja.deviceapi.RFIDWithISO15693.TagType
getVersion() - Method in class com.rscja.deviceapi.Fingerprint
  获取模块版本
  Acquire module version
getVersion() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取模块版本
  Acquire module version
getVersion() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
getVersion() - Method in interface com.rscja.deviceapi.interfaces.IRFIDBase
  获取rfid 版本信息
  Acquire RFID version infor
getVersion() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  读取UHF模块版本号
  Read UHF module version
getVersion() - Method in class com.rscja.deviceapi.Printer
getVersion() - Method in class com.rscja.deviceapi.RFIDBase
  获取rfid 版本信息
  Acquire RFID version infor
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  读取UHF模块版本号(Read UHF module version)
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  读取UHF模块版本号(Read UHF module version)
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  读取UHF模块版本号(Read UHF module version)
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  读取UHF模块版本号(Read UHF module version)
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  读取UHF模块版本号
  Read UHF module version
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getVersion() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
getVersion() - Static method in class com.rscja.deviceapi.VersionInfo
  获取jar包版本信息
  acquire jar pack version infor
getVersions() - Method in class com.rscja.deviceapi.FingerprintWithFIPS.FingerprintInfo
  获取指纹模块版本号
  Acquire fingerprint module version
getVersionSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
getWifiInfo() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getWifiInfo() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取wifi热点信息,json格式数据
getWifiInfo() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取wifi热点信息,json格式数据
getWifiInfo() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取wifi热点信息,json格式数据
getWifiInfo() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取wifi热点信息,json格式数据
getWifiIpConfig() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
getWifiIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取wifi配置信息
getWifiIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取wifi配置信息
getWifiIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取wifi配置信息
getWifiIpConfig() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取wifi配置信息
getWorkMode() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  获取工作模式
getWorkMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
getWorkMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取工作模式
getWorkMode() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
getWorkModeSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParseUrx
getWritePermissions() - Method in class com.rscja.deviceapi.entity.DESFireFile
  获取写权限
  acquire write authorization
getWriteSendData(String, int, int, int, String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
  获取写标签的发送数据
GPI1 - Static variable in class com.rscja.deviceapi.entity.GPIStateEntity
GPI2 - Static variable in class com.rscja.deviceapi.entity.GPIStateEntity
GPI3 - Static variable in class com.rscja.deviceapi.entity.GPIStateEntity
GPI4 - Static variable in class com.rscja.deviceapi.entity.GPIStateEntity
GPIOInfo - Class in com.rscja.deviceapi.entity
GPIOInfo() - Constructor for class com.rscja.deviceapi.entity.GPIOInfo
GPIStateEntity - Class in com.rscja.deviceapi.entity
GPIStateEntity() - Constructor for class com.rscja.deviceapi.entity.GPIStateEntity
GPIStateEntity(String, int) - Constructor for class com.rscja.deviceapi.entity.GPIStateEntity
GPO1 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
GPO2 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
GPO3 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
GPO4 - Static variable in class com.rscja.deviceapi.entity.GPOEntity
GPOEntity - Class in com.rscja.deviceapi.entity
GPOEntity(String, int) - Constructor for class com.rscja.deviceapi.entity.GPOEntity
grab() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  采集图像
  Acquire image
grab() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  采集图像
  Acquire image

A B C D E F G H I K L M N O P R S T U V W Z