A B C D E F G H I K L M N O P R S T U V W Z

## E

EM125k_ReadHitag1() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  获取所有页的数据
  Acquire data of all pages
EM125k_ReadHitag1() - Method in class com.rscja.deviceapi.RFIDWithLF
  获取所有页的数据
  Acquire data of all pages
empty() - Method in class com.rscja.deviceapi.Fingerprint
  清空模块中保存的指纹数据
  empty out saved fingerprint data in module.
empty() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  清空模块中保存的指纹数据
  empty out saved fingerprint data in module.
enableAuxiliaryLight(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  开启扫描辅助灯(C7x才有此功能)
  switch on scanning aux.light for C7x series
enableAuxiliaryLight(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
enableBarcodeNotRepeat(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  不输出重复标签(前后两次标签不重复)
  donot outout repeated tags
enableBarcodeNotRepeat(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
enableBeep() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
enableBeep() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  启用蜂鸣器
enableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  启用蜂鸣器，打开蜂鸣器后盘点到标签会响应蜂鸣器。(Turn the buzzer on, and the label will respond to the buzzer after turning on the buzzer.)
enableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  启用蜂鸣器，打开蜂鸣器后盘点到标签会响应蜂鸣器。(Turn the buzzer on, and the label will respond to the buzzer after turning on the buzzer.)
enableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  启用蜂鸣器，打开蜂鸣器后盘点到标签会响应蜂鸣器。(Turn the buzzer on, and the label will respond to the buzzer after turning on the buzzer.)
enableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  启用蜂鸣器，打开蜂鸣器后盘点到标签会响应蜂鸣器。(Turn the buzzer on, and the label will respond to the buzzer after turning on the buzzer.)
enableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
enableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  启用蜂鸣器
enableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
enableBlockScankey(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  拦截扫描按键 (备注：键盘助手v2.3.5 之后的版本才支持)
  Block scan button (Comment: Supports after keyboardemualator v2.3.5 has been released)
enableBlockScankey(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
enableContinuousScan(Context, boolean) - Method in class com.rscja.barcode.BarcodeUtility
  启用连续扫描 Enable continuous scan
enableContinuousScan(Context, boolean) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  启用连续扫描 Enable continuous scan
enableEnter(Context, boolean) - Method in class com.rscja.barcode.BarcodeUtility
  是否启用回车 Whether enable Enter function
enableEnter(Context, boolean) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  是否启用回车 Whether enable Enter function
enableEnter(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  是否启用回车
  Enter ON/OFF
enableEnter(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
enableFunction(Context, int) - Method in interface com.rscja.scanner.IScanner
  启用指定功能模块
  Enable specific function module
enableFunction(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
enablePlayFailureSound(Context, boolean) - Method in class com.rscja.barcode.BarcodeUtility
  扫描失败是否播放提示音 whether playing notification when scanning failure.
enablePlayFailureSound(Context, boolean) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  扫描失败是否播放提示音 whether playing notification when scanning failure.
enablePlayFailureSound(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  扫描失败是否播放提示音
  scan failure sound ON/OFF
enablePlayFailureSound(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
enablePlaySuccessSound(Context, boolean) - Method in class com.rscja.barcode.BarcodeUtility
  是否播放成功的提示音 whether playing notification when scanning success.
enablePlaySuccessSound(Context, boolean) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  是否播放成功的提示音 whether playing notification when scanning success.
enablePlaySuccessSound(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  扫描成功是否播放提示音
  Scan success sound ON/OFF
enablePlaySuccessSound(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
enableScanOnRelease(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  释放扫描按键开始扫描
enableScanOnRelease(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
  释放扫描按键开始扫描
enableTAB(Context, boolean) - Method in class com.rscja.barcode.BarcodeUtility
  是否启用TAB Whether enable TAB function
enableTAB(Context, boolean) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  是否启用TAB Whether enable TAB function
enableTAB(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  是否启用TAB
  TAB ON/OFF
enableTAB(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
enableVibrate(Context, boolean) - Method in class com.rscja.barcode.BarcodeUtility
  扫描成功是否震动提示 whether vibrating when scanning success
enableVibrate(Context, boolean) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  扫描成功是否震动提示 whether vibrating when scanning success
enableVibrate(Context, boolean) - Method in interface com.rscja.scanner.IScanner
  扫描成功是否震动提示
  scan success vibrate ON/OFF
enableVibrate(Context, boolean) - Method in class com.rscja.scanner.utility.ScannerUtility
enroll() - Method in class com.rscja.deviceapi.FingerprintSM206B
  录入指纹，用户录入 3~5 次指纹，生成 256 字节指纹特征值
enroll() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  采集指纹
  Acquire fingerprint
enroll() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintSM206B
enroll() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  采集指纹
  Acquire fingerprint
eraseData(String, int, int, int, String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  擦除指定标签的数据，被擦除的数据块其内容将被设置成0.
  Clean specific tag data, data block after cleaned will be set to 0.
eraseData(String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  擦除数据，被擦除的数据块其内容将被设置成0.
  Data block that has been cleaned will be setup to 0.
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  擦除指定标签的数据，被擦除的数据块其内容将被设置成0.(Clean specific tag data, data block after cleaned will be set to 0.
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  擦除数据，被擦除的数据块其内容将被设置成0.
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  擦除指定标签的数据，被擦除的数据块其内容将被设置成0.(Clean specific tag data, data block after cleaned will be set to 0.
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  擦除数据，被擦除的数据块其内容将被设置成0.
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  擦除指定标签的数据，被擦除的数据块其内容将被设置成0.(Clean specific tag data, data block after cleaned will be set to 0.
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  擦除数据，被擦除的数据块其内容将被设置成0.
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  擦除指定标签的数据，被擦除的数据块其内容将被设置成0.(Clean specific tag data, data block after cleaned will be set to 0.
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  擦除数据，被擦除的数据块其内容将被设置成0.
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  擦除指定标签的数据，被擦除的数据块其内容将被设置成0.
  Clean specific tag data, data block after cleaned will be set to 0.
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  擦除数据，被擦除的数据块其内容将被设置成0.
  Data block that has been cleaned will be setup to 0.
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
eraseData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
eraseData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
eraseFlash() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
eraseFlash() - Method in class com.rscja.deviceapi.Printer
eraseFW(long) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
eraseFW(long) - Method in class com.rscja.deviceapi.Printer
ERRCODE_FAILURE - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  失败(Failure)
ERRCODE_SUCCESS - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  成功(Success)
ERROR_INSUFFICIENT_PRIVILEGES - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  没有权限访问(The Interrogator did not authenticate itself with sufficient privileges for the Tag to perform the operation)
ERROR_MEMORY_LOCK - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  数据区被锁定(Memory lock)
ERROR_MEMORY_OVERRUN - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  数据区超限(Memory Overflow)
ERROR_NO_ENOUGH_POWER_ON_TAG - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  标签能量不足(no enough power on tag)
ERROR_NO_TAG - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  找不到标签(No tags found.)
ERROR_OPERATION_FAILED - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  操作失败(0peration failure)
ERROR_PASSWORD_IS_INCORRECT - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  密码不正确(Incorrect Password)
ERROR_RECV_FAIL - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  接收失败(Receive failure)
ERROR_RESPONSE_BUFFER_OVERFLOW - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  缓冲区溢出(The operation failed because the ResponseBuffer overflowed)
ERROR_SEND_FAIL - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  发送失败(Send failure)
ERROR_TAG_NO_REPLY - Static variable in class com.rscja.deviceapi.UhfBase.ErrorCode
  标签没有应答(Tag not responding)
ErrorCode() - Constructor for class com.rscja.deviceapi.UhfBase.ErrorCode
executeCmd(String, String) - Method in interface com.rscja.deviceapi.interfaces.IPSAM
  执行PSAM命令
  Execute PSAM command
executeCmd(String, String) - Method in class com.rscja.deviceapi.PSAM
  执行PSAM命令
  Execute PSAM command
exists(int) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  检查指定的编号是否已被注册
exists(int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  检查指定的编号是否已被注册
EXTRADATA_EPCAREA - Variable in class com.rscja.deviceapi.entity.UHFTAGInfo

A B C D E F G H I K L M N O P R S T U V W Z