A B C D E F G H I K L M N O P R S T U V W Z

## R

R1HFAndPsamManage - Class in com.rscja.deviceapi
  R1设备高频和PSAM操作类
  R1 device HF and PSAM operation interfaces
  第一步:通过`R1HFAndPsamManage.connect(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`R1HFAndPsamManage.connect(Context context)`
  第二步:获取相关接口对象`R1HFAndPsamManage.getHF14443A()`、`R1HFAndPsamManage.getHF14443B()`、`R1HFAndPsamManage.getHF15693()`、`R1HFAndPsamManage.getPSAM()`
  Step 2:Gets the associated interface object `R1HFAndPsamManage.getHF14443A()`、`R1HFAndPsamManage.getHF14443B()`、`R1HFAndPsamManage.getHF15693()`、`R1HFAndPsamManage.getPSAM()`
  Example Usage:
  public void HFDemo() {   R1HFAndPsamManage rfid = R1HFAndPsamManage.getInstance();   if (!rfid.connect(context)) {    //fail    return;   }   IHF14443A ihf14443A = rfid.getHF14443A();   IHF14443B ihf14443B = rfid.getHF14443B();   IHF15693 ihf15693 = rfid.getHF15693();   IPSAM ipsam = rfid.getPSAM();   HF14443RequestEntity entity = ihf14443A.requestTypeA();   if (entity == null) {    //"Card not found!"    return;   }   byte cMode = 0x60:A ; 0x61:B   byte cBlock;   byte[] txtKey;//6bytes   boolean reuslt = ihf14443A.authentication(cMode, cBlock, txtKey);   if (!reuslt) {    //The key validation fail    return;   }   //................
rats() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A4CPU
  CPU卡RATS操作指令
  CPU card RATS operation command
rats() - Method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  CPU卡RATS操作指令
  CPU card RATS operation command
ratsTypeA() - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  CPU卡RATS操作指令(CPU card RATS operation command)
read(HF15693RequestEntity, int) - Method in interface com.rscja.deviceapi.interfaces.IHF15693
  读卡(Read card)
read(String, RFIDWithISO14443A.KeyType, int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  读卡,此函数包含寻卡和验证密钥步骤
  Read card, this formula includes card search and key verfication procedure
read(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  读卡，适用于Urltra light标签
  card reading, used for Urltra light tag
read(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  读取块数据
  read block data
read(int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  读取块数据
  block data
read(String, RFIDWithISO14443A.KeyType, int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读卡,此函数包含寻卡和验证密钥步骤
  Read card, this formula includes card search and key verfication procedure
read(int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读卡，适用于Urltra light标签
  card reading, used for Urltra light tag
read(int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  读取块数据
  read block data
read(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO15693
  读取块数据
  block data
readAllData(String, RFIDWithISO14443A.TagType) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  读卡，读取卡片所有块中的数据
  Card reading, read data of all blocks in the card
readAllData(String, RFIDWithISO14443A.TagType) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读卡，读取卡片所有块中的数据
  Card reading, read data of all blocks in the card
readAnimalTags(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读取动物标签信息
  read animal tag infor
readAnimalTags(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读取动物标签信息
  read animal tag infor
readBlock(byte) - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  读卡(Read card)
readChipSN() - Method in class com.rscja.deviceapi.Fingerprint
  获取芯片序列号
  acquire chip serial number
readChipSN() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取芯片序列号
  acquire chip serial number
readData(String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
readData(String, int, int, int, String) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
readData(String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  读取标签数据
  Read tag data
readData(String, int, int, int, String, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  读取指定标签数据
  Read specific tag data
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  读取标签的数据(Read tag data)
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  读取指定标签的数据(Read the data of the specified tag)
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  读取标签的数据(Read tag data)
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  读取指定标签的数据(Read the data of the specified tag)
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  读取标签的数据(Read tag data)
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  读取指定标签的数据(Read the data of the specified tag)
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  读取标签的数据(Read tag data)
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  读取指定标签的数据(Read the data of the specified tag)
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
readData(String, int, int, int, String) - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  读取标签数据
  Read tag data
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  读取指定标签数据
  Read specific tag data
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
readData(String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
readData(String, int, int, int, String, int, int, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
readDataWith4305Card(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读4305卡的某一页（0~31）数据
  read card 4305 data of random page (0-31)
readDataWith4305Card(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读4305卡的某一页（0~31）数据
  read card 4305 data of random page (0-31)
readDataWithHitagS(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读取Hitag S卡中的某一页的数据
  Read data of random page in Hitag S card
readDataWithHitagS(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读取Hitag S卡中的某一页的数据
  Read data of random page in Hitag S card
readDataWithIDCard(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读卡,用于ID卡
  card reading, used for ID card
readDataWithIDCard(int) - Method in class com.rscja.deviceapi.RFIDWithLF
  读卡,用于ID卡
  card reading, used for ID card
ReaderIPEntity - Class in com.rscja.deviceapi.entity
ReaderIPEntity() - Constructor for class com.rscja.deviceapi.entity.ReaderIPEntity
ReaderIPEntity(String, int) - Constructor for class com.rscja.deviceapi.entity.ReaderIPEntity
readSysPara() - Method in class com.rscja.deviceapi.Fingerprint
  获取系统参数，仅返回版本号
  Acquire system parameter, return version number only
readSysPara() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取系统参数，仅返回版本号
  Acquire system parameter, return version number only
readSysParaMore() - Method in class com.rscja.deviceapi.Fingerprint
  获取系统参数
  Acquire system parameter
readSysParaMore() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  获取系统参数
  Acquire system parameter
readTagFromBuffer() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  获取缓冲区的标签数据
  Get tag data from buffer
  `IUHF.startInventoryTag()`启动识别标签之后，在子线程循环调用此函数不断获取缓冲区的标签信息，每次返回一张标签数据
  `IUHF.startInventoryTag()` After tag reading has been enabled, call this function in sub threads to get data information continously, return one tag information for each time.
  在调用`IUHF.stopInventory()`之后，应当退出子线程。
  After call `IUHF.stopInventory()`, exit sub threads.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  接收循环盘点的标签数据
  Receive label data for cycle count
  创建一个子线程调用此方法获取标签数据，此方法非阻塞模式。此方法只负责从数据缓冲区获取标签数据，如果数据缓冲区没有标签数据，将返回NULL。
  Create a child thread to call this method to get tag data, this method is non-blocking mode.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  接收循环盘点的标签数据
  Receive label data for cycle count
  创建一个子线程调用此方法获取标签数据，此方法非阻塞模式。此方法只负责从数据缓冲区获取标签数据，如果数据缓冲区没有标签数据，将返回NULL。
  Create a child thread to call this method to get tag data, this method is non-blocking mode.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  接收循环盘点的标签数据
  Receive label data for cycle count
  创建一个子线程调用此方法获取标签数据，此方法非阻塞模式。此方法只负责从数据缓冲区获取标签数据，如果数据缓冲区没有标签数据，将返回NULL。
  Create a child thread to call this method to get tag data, this method is non-blocking mode.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  接收循环盘点的标签数据
  Receive label data for cycle count
  创建一个子线程调用此方法获取标签数据，此方法非阻塞模式。此方法只负责从数据缓冲区获取标签数据，如果数据缓冲区没有标签数据，将返回NULL。
  Create a child thread to call this method to get tag data, this method is non-blocking mode.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  获取缓冲区的标签数据
  Get tag data from buffer
  `RFIDWithUHFUrxUart.startInventoryTag()`启动识别标签之后，在子线程循环调用此函数不断获取缓冲区的标签信息，每次返回一张标签数据
  `RFIDWithUHFUrxUart.startInventoryTag()` After tag reading has been enabled, call this function in sub threads to get data information continously, return one tag information for each time.
  在调用`RFIDWithUHFUrxUart.stopInventory()`之后，应当退出子线程。
  After call `RFIDWithUHFUrxUart.stopInventory()`, exit sub threads.
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
readTagFromBuffer() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
readTagFromBufferList() - Method in interface com.rscja.deviceapi.interfaces.IUhfReader
  获取缓冲区的标签数据
  Acquire tag data in buffer
  `#startInventoryTag()` 启动识别标签之后，在子线程循环调用此函数不断获取缓冲区的标签信息，此函数只返回EPC数据
  `#startInventoryTag()` after enable identify tag, acquire tag information in buffer by this function in sub thread, this fucntion will return EPC data only
  在调用`#stopInventory()` 之后，应当退出子线程。
  after call `#stopInventory()` , exit sub tread.
readTagFromBufferList() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  获取缓冲区的标签数据
  Acquire tag data in buffer
  `RFIDWithUHFBLE.startInventoryTag()`启动识别标签之后，在子线程循环调用此函数不断获取缓冲区的标签信息，此函数只返回EPC数据
  `RFIDWithUHFBLE.startInventoryTag()` after enable identify tag, acquire tag information in buffer by this function in sub thread, this fucntion will return EPC data only
  在调用`RFIDWithUHFBLE.stopInventory()`之后，应当退出子线程。
  after call `RFIDWithUHFBLE.stopInventory()`, exit sub tread.
  备注： 读写器主板版 2.20-2.29 此函数支持输出Rssi,不需要调用readTagFromBufferList_EpcTidUser
readTagFromBufferList() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
readTagFromBufferList_EpcTidUser() - Method in interface com.rscja.deviceapi.interfaces.IUhfBle
readTagFromBufferList_EpcTidUser() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  Deprecated.
readUnsignedInt64(byte[]) - Static method in class com.rscja.utility.StringUtility
  读取无符号位的长整数，64位
readWithNeedleTag() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  读数据，针对针管标签
  read data, for needle tube tag
readWithNeedleTag() - Method in class com.rscja.deviceapi.RFIDWithLF
  读数据，针对针管标签
  read data, for needle tube tag
readyUpgradeTcpService() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
readyUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  升级UHF Tcp服务器程序第一步,准备升级TCP服务程序
readyUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  升级UHF Tcp服务器程序第一步,准备升级TCP服务程序
readyUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  升级UHF Tcp服务器程序第一步,准备升级TCP服务程序
readyUpgradeTcpService() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  升级UHF Tcp服务器程序第一步,准备升级TCP服务程序
rebootDevice() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
rebootDevice() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  重启设备
rebootDevice() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  重启设备
rebootDevice() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  重启设备
rebootDevice() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  重启设备
receive(byte[]) - Method in interface com.rscja.deviceapi.BluetoothReader.OnDataChangeListener
receive() - Method in class com.rscja.deviceapi.Infrared
  接收数据
  Receive data
receive(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothData.OnBleDataChangeListener
receive() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  接收数据
  Receive data
receive() - Method in interface com.rscja.deviceapi.interfaces.IModule
  接收数据,读取串口数据会等待1秒钟
  Receive data
receive() - Method in class com.rscja.deviceapi.Module
  接收数据,读取串口数据会等待1秒钟
  Receive data
receiveData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  接收串口数据
  receive serial port data
receiveData(byte[]) - Method in class com.rscja.deviceapi.Printer
  接收串口数据
  receive serial port data
receiveEx() - Method in interface com.rscja.deviceapi.interfaces.IModule
  接收数据,读取串口数据无等待时间
  Receive data
receiveEx() - Method in class com.rscja.deviceapi.Module
  接收数据,读取串口数据无等待时间
  Receive data
regModel() - Method in class com.rscja.deviceapi.Fingerprint
  合并特征文件。将模板缓冲区1与模板缓冲区2中的模板文件合并生成模板，结果存于模板缓冲区1。
  Combine feature file.
regModel() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  合并特征文件。将模板缓冲区1与模板缓冲区2中的模板文件合并生成模板，结果存于模板缓冲区1。
  Combine feature file.
releasePrinterGpio() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
releasePrinterGpio() - Method in class com.rscja.deviceapi.Printer
removeLiveAPP(String[]) - Method in interface com.rscja.system.ISystemInterfaces
  移除保活APP
request() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  寻卡
  Search card
request() - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  寻卡
  Search card
request15693() - Method in interface com.rscja.deviceapi.interfaces.IHF15693
  寻卡(Search card)
requestTypeA() - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  寻卡(Search card)
requestTypeA(int) - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  寻卡(Search card)
reset() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A4CPU
  CPU卡复位操作指令
  CPU card reset operation command
reset() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443B
  CPU卡复位操作指令
  CPU card reset operation commande
reset() - Method in class com.rscja.deviceapi.RFIDWithISO14443A4CPU
  CPU卡复位操作指令
  CPU card reset operation command
reset() - Method in class com.rscja.deviceapi.RFIDWithISO14443B
  CPU卡复位操作指令
  CPU card reset operation commande
resetScan(Context) - Method in interface com.rscja.scanner.IScanner
  键盘助手恢复出厂设置
  Restore factory setup
resetScan(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
resetTypeB() - Method in interface com.rscja.deviceapi.interfaces.IHF14443B
  寻卡(Search card)
responseCancel() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  取消当前操作
  Cancel current operation
responseCancel() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  取消当前操作
  Cancel current operation
responseContinue() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  继续当前操作
  Continue current operation
responseContinue() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  继续当前操作
  Continue current operation
restoreDefault() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  参数还原默认值
  parameter reset to default
restoreDefault() - Method in class com.rscja.deviceapi.Printer
  参数还原默认值
  parameter reset to default
RESULT_STATUS - Static variable in class com.idata.scanner.decoder.ConstantUtil
reverse(byte[]) - Static method in class com.rscja.utility.StringUtility
  逆转字节数组
RFIDArgumentException - Exception in com.rscja.deviceapi.exception
  参数错误异常
  parameter err
RFIDArgumentException(String) - Constructor for exception com.rscja.deviceapi.exception.RFIDArgumentException
RFIDBase - Class in com.rscja.deviceapi
RFIDBase() - Constructor for class com.rscja.deviceapi.RFIDBase
RFIDNotFoundException - Exception in com.rscja.deviceapi.exception
  寻卡失败异常
  card searching failed err
RFIDNotFoundException() - Constructor for exception com.rscja.deviceapi.exception.RFIDNotFoundException
RFIDReadFailureException - Exception in com.rscja.deviceapi.exception
  读卡失败异常
  card reading failure err
RFIDReadFailureException() - Constructor for exception com.rscja.deviceapi.exception.RFIDReadFailureException
rfidUpgrade(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IRFIDBase
  固件升级
  firmware upgrade
rfidUpgrade(int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDBase
  固件升级
  firmware upgrade
RFIDVerificationException - Exception in com.rscja.deviceapi.exception
  验证失败异常
  verify failure err
RFIDVerificationException() - Constructor for exception com.rscja.deviceapi.exception.RFIDVerificationException
RFIDWithISO14443A - Class in com.rscja.deviceapi
  RFID模块ISO14443A协议操作类
  RFID module ISO 14443A protocol operation type
RFIDWithISO14443A.DESFireEncryptionTypekEnum - Enum in com.rscja.deviceapi
  DESFire卡加密类型
  DESFire card encyption type
RFIDWithISO14443A.DESFireFileTypekEnum - Enum in com.rscja.deviceapi
  DESFire卡文件类型
  DESFire card file typr
RFIDWithISO14443A.KeyType - Enum in com.rscja.deviceapi
  密钥类型，适用于S50和S70标签。
  key type, used for S50 and S70 tags.
RFIDWithISO14443A.TagType - Enum in com.rscja.deviceapi
  M1标签类型定义
  M1 tag type definition
RFIDWithISO14443A4CPU - Class in com.rscja.deviceapi
  RFID模块ISO14443A CPU卡协议操作类
  RFID module ISO14443A CPU card protocol operation type
RFIDWithISO14443B - Class in com.rscja.deviceapi
  RFID模块ISO14443B协议操作类
  RFID module ISO14443B protocol operation type
RFIDWithISO15693 - Class in com.rscja.deviceapi
  RFID模块ISO15693协议操作类,
  RFID module ISO15639 protocol operation type
RFIDWithISO15693.TagType - Enum in com.rscja.deviceapi
  标签类型
  Tag type
RFIDWithLF - Class in com.rscja.deviceapi
  RFID低频（125K）操作类
  RFID LF (125K) operation type
RFIDWithUHFA4 - Class in com.rscja.deviceapi
  UHF模块 A4操作类
  UHF module operation type
  第一步:通过`RFIDWithUHFUART.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUART.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUART.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUART.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFA4NetWork - Class in com.rscja.deviceapi
  操作URA4设备以及UHF模块相关接口。(通过其他android设备控制A4)
  Operate URA4 devices and related interfaces of UHF modules.
  操作步骤：
  Steps:
  第一步：先通过`RFIDWithUHFA4NetWork.setIPAndPort(String ip, int port)`设置要连接的IP地址, 再通过 `RFIDWithUHFA4NetWork.init(Context context)`连接读写器串口。同时可以设置回调接口 `RFIDWithUHFA4NetWork.setConnectionStatusCallback(ConnectionStatusCallback btStateCallback)`监听连接状态。
  Step 1: Connect to the serial port of the reader via`RFIDWithUHFA4NetWork.setIPAndPort(String ip, int port)`-> `RFIDWithUHFA4NetWork.init(Context context)`.
RFIDWithUHFA4NetWork() - Constructor for class com.rscja.deviceapi.RFIDWithUHFA4NetWork
RFIDWithUHFA4RS232 - Class in com.rscja.deviceapi
  操作URA4设备以及UHF模块相关接口。(通过其他android设备控制A4)
  Operate URA4 devices and related interfaces of UHF modules.
  操作步骤：
  Steps:
  第一步：先通过`RFIDWithUHFA4RS232.setUart(String path)`设置要连接的IP地址, 再通过 `RFIDWithUHFA4RS232.init(Context context)`连接读写器串口。同时可以设置回调接口 `RFIDWithUHFA4RS232.setConnectionStatusCallback(ConnectionStatusCallback btStateCallback)`监听连接状态。
  Step 1: Connect to the serial port of the reader via`RFIDWithUHFA4RS232.setUart(String path)`-> `RFIDWithUHFA4RS232.init(Context context)`.
RFIDWithUHFA8 - Class in com.rscja.deviceapi
  UHF模块 A8操作类
  UHF module operation type
  第一步:通过`RFIDWithUHFUART.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUART.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUART.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUART.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFA8NetWork - Class in com.rscja.deviceapi
  操作URA8设备以及UHF模块相关接口。(通过其他android设备控制A8)
  Operate URA8 devices and related interfaces of UHF modules.
  操作步骤：
  Steps:
  第一步：先通过`RFIDWithUHFA8NetWork.setIPAndPort(String ip, int port)`设置要连接的IP地址, 再通过 `RFIDWithUHFA8NetWork.init(Context context)`连接读写器串口。同时可以设置回调接口 `RFIDWithUHFA8NetWork.setConnectionStatusCallback(ConnectionStatusCallback btStateCallback)`监听连接状态。
  Step 1: Connect to the serial port of the reader via`RFIDWithUHFA8NetWork.setIPAndPort(String ip, int port)`-> `RFIDWithUHFA8NetWork.init(Context context)`.
RFIDWithUHFA8NetWork() - Constructor for class com.rscja.deviceapi.RFIDWithUHFA8NetWork
RFIDWithUHFA8RS232 - Class in com.rscja.deviceapi
  操作URA8设备以及UHF模块相关接口。(通过其他android设备控制A8)
  Operate URA8 devices and related interfaces of UHF modules.
  操作步骤：
  Steps:
  第一步：先通过`RFIDWithUHFA8RS232.setUart(String path)`设置要连接的IP地址, 再通过 `RFIDWithUHFA8RS232.init(Context context)`连接读写器串口。同时可以设置回调接口 `RFIDWithUHFA8RS232.setConnectionStatusCallback(ConnectionStatusCallback btStateCallback)`监听连接状态。
  Step 1: Connect to the serial port of the reader via`RFIDWithUHFA8RS232.setUart(String path)`-> `RFIDWithUHFA8RS232.init(Context context)`.
RFIDWithUHFAxBase - Class in com.rscja.deviceapi
RFIDWithUHFBLE - Class in com.rscja.deviceapi
  UHF模块低功耗蓝牙操作类
  UHF module operation type
RFIDWithUHFRLM - Class in com.rscja.deviceapi
RFIDWithUHFUART - Class in com.rscja.deviceapi
  UHF模块手持机，串口通信操作类
  UHF module handheld, serial communication operation interface
  第一步:通过`RFIDWithUHFUART.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUART.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUART.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUART.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFUrxNetwork - Class in com.rscja.deviceapi
  UHF模块URx网口通信操作类
  URx network operation of UHF module
  第一步：先通过`RFIDWithUHFUrxNetwork.setIPAndPort(String ip, int port)`设置要连接的IP地址, 再通过 `RFIDWithUHFUrxNetwork.init(Context context)`连接读写器串口。 Step 1: Connect to the serial port of the reader via`RFIDWithUHFUrxNetwork.setIPAndPort(String ip, int port)`-> `RFIDWithUHFUrxNetwork.init(Context context)`.
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUrxNetwork.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUrxNetwork.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFUrxNetwork() - Constructor for class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
RFIDWithUHFUrxUart - Class in com.rscja.deviceapi
  URx 模块，串口通信操作类
  URx module , serial communication operation interface
  第一步:通过`RFIDWithUHFUrxUart.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUrxUart.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUrxUart.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUrxUart.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFUrxUsbToUart - Class in com.rscja.deviceapi
  URx 模块，串口通信操作类
  URx module , serial communication operation interface
  第一步:通过`RFIDWithUHFUrxUsbToUart.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUrxUsbToUart.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUrxUsbToUart.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUrxUsbToUart.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.
RFIDWithUHFUSB - Class in com.rscja.deviceapi
  UHF模块手持机，USB通信操作类
  UHF module handheld, USB operation interface
  第一步:通过`RFIDWithUHFUSB.init(Context context)` 连接读写器。
  Step 1: Connect to the usb of the reader via`RFIDWithUHFUSB.init(Context context)`
  第二步： 如果是设置参数，连接成功之后，调用对应的函数设置参数、读写操作。 如果是盘点调用`RFIDWithUHFUSB.startInventoryTag()`函数开始执行盘点。 注意: 在盘点标签的时候rfid模块只能响应`RFIDWithUHFUSB.stopInventory()`函数。
  Step 2: If it is to set parameters, after the connection is successful, call the corresponding function to set parameters, read and write operations.

A B C D E F G H I K L M N O P R S T U V W Z