A B C D E F G H I K L M N O P R S T U V W Z

## C

C5_6765 - Static variable in class com.rscja.CWDeviceInfo
C6000_6735 - Static variable in class com.rscja.CWDeviceInfo
C6000_6762 - Static variable in class com.rscja.CWDeviceInfo
C60_MTK_6765_110 - Static variable in class com.rscja.CWDeviceInfo
C60_QCM2150_100 - Static variable in class com.rscja.CWDeviceInfo
C60_SMD450_100 - Static variable in class com.rscja.CWDeviceInfo
C61_SMD450_90 - Static variable in class com.rscja.CWDeviceInfo
C61P_SM6115_110 - Static variable in class com.rscja.CWDeviceInfo
C66_8953 - Static variable in class com.rscja.CWDeviceInfo
C66_SMD450_90 - Static variable in class com.rscja.CWDeviceInfo
C66P_SM6115_110 - Static variable in class com.rscja.CWDeviceInfo
C70_6735 - Static variable in class com.rscja.CWDeviceInfo
C70_6763 - Static variable in class com.rscja.CWDeviceInfo
C70_6765 - Static variable in class com.rscja.CWDeviceInfo
C71_6763 - Static variable in class com.rscja.CWDeviceInfo
C71_6765 - Static variable in class com.rscja.CWDeviceInfo
C72_6735 - Static variable in class com.rscja.CWDeviceInfo
C72_6763 - Static variable in class com.rscja.CWDeviceInfo
C72_6765 - Static variable in class com.rscja.CWDeviceInfo
C75_6765 - Static variable in class com.rscja.CWDeviceInfo
C76_6735 - Static variable in class com.rscja.CWDeviceInfo
C76_6765 - Static variable in class com.rscja.CWDeviceInfo
C90_6762_10 - Static variable in class com.rscja.CWDeviceInfo
callback(List<GPIStateEntity>) - Method in interface com.rscja.deviceapi.interfaces.IGPIStateCallback
callback(UHFTAGInfo) - Method in interface com.rscja.deviceapi.interfaces.IUHFInventoryCallback
cardConsumeConfirm(String, String, String) - Method in class com.rscja.deviceapi.CardWithBYL
cardConsumeConfirm(String, String, String) - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
CardWithBYL - Class in com.rscja.deviceapi
  白玉兰公交卡操作类
char2HexString(char) - Static method in class com.rscja.utility.StringUtility
  char转十六进制
charArrayTolong(char[]) - Static method in class com.rscja.utility.StringUtility
  将8字节的Char数组转成一个long值
chars2HexString(char[], int) - Static method in class com.rscja.utility.StringUtility
  char类型数组转十六进制字符串
chars2Long(char[], int, int) - Static method in class com.rscja.utility.StringUtility
  char数组转long
charsTobytes(char[], int) - Static method in class com.rscja.utility.StringUtility
checkData(List<Byte>) - Method in class com.rscja.deviceapi.UHFProtocolParseBase
checkParameter() - Method in class com.rscja.deviceapi.entity.Gen2Entity
cleanFaultCard() - Method in class com.rscja.deviceapi.CardWithBYL
  清除故障卡
cleanFaultCard() - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  清除故障卡
clearCache() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  立即清空打印缓存,清空打印机接收缓冲区和打印缓冲区
  Clear up printing cache, clear printer receive zone and buffer zone
clearCache() - Method in class com.rscja.deviceapi.Printer
  立即清空打印缓存,清空打印机接收缓冲区和打印缓冲区
  Clear up printing cache, clear printer receive zone and buffer zone
close() - Method in class com.rscja.barcode.BarcodeDecoder
  关闭二维扫描设备
  Switch off 2D barcode scannning device
close(Context, BarcodeUtility.ModuleType) - Method in class com.rscja.barcode.BarcodeUtility
  关闭指定功能 Switch off designated function
close() - Method in class com.rscja.deviceapi.Barcode1D
  关闭一维扫描设备
  Switch off 1D barcode scanning device.
close() - Method in class com.rscja.deviceapi.Barcode2D
  关闭二维扫描设备
  Switch off 2D barcode scanning device.
close() - Method in class com.rscja.deviceapi.Infrared
  关闭红外模块
  Switch off infared module
close() - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
  关闭一维扫描设备
  Switch off 1D barcode scanning device.
close() - Method in interface com.rscja.deviceapi.interfaces.IBarcode2D
  关闭二维扫描设备
  Switch off 2D barcode scanning device.
close(Context, BarcodeUtility.ModuleType) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  关闭指定功能 Switch off designated function
close() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  关闭红外模块
  Switch off infared module
close() - Method in interface com.rscja.deviceapi.interfaces.ILedLight
  关闭LED灯
  Switch off LED
close() - Method in interface com.rscja.deviceapi.interfaces.IZebra2DSoftDecoder
close() - Method in class com.rscja.deviceapi.LedLight
  关闭LED灯
  Switch off LED
close(Context) - Method in interface com.rscja.scanner.IScanner
  关闭键盘助手总开关
  Switch off keyboardemulator
close(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
closeAuxiliaryLight(Context) - Method in interface com.rscja.deviceapi.interfaces.IScanerLedLight
  关闭扫描辅助灯，目前只支持C70系列
  Switch on scanning light, support C70 series only
closeAuxiliaryLight(Context) - Method in class com.rscja.deviceapi.ScanerLedLight
closeKeyboardHelper(Context) - Method in class com.rscja.barcode.BarcodeUtility
  关闭键盘助手功能总开关 Switch off main function switch of keyboardemulator
closeKeyboardHelper(Context) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  关闭键盘助手功能总开关 Switch off main function switch of keyboardemulator
closeLed() - Method in class com.rscja.deviceapi.BluetoothReader
  关闭led
closeLED() - Method in class com.rscja.deviceapi.Infrared
  关闭辅助灯
  Close LED
closeLED() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
  关闭辅助灯
  Close LED
closeLed() - Method in interface com.rscja.deviceapi.interfaces.IReader
  关闭led
closeLed() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  关闭led
closeLedSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
closeSerail() - Method in interface com.rscja.deviceapi.interfaces.IModule
  关闭串口
closeSerail() - Method in class com.rscja.deviceapi.Module
  关闭串口
closeWifi() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
closeWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  关闭wifi
closeWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  关闭wifi
closeWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  关闭wifi
closeWifi() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  关闭wifi
com.idata.scanner.decoder - package com.idata.scanner.decoder
com.rscja.barcode - package com.rscja.barcode
com.rscja.deviceapi - package com.rscja.deviceapi
com.rscja.deviceapi.entity - package com.rscja.deviceapi.entity
com.rscja.deviceapi.enums - package com.rscja.deviceapi.enums
com.rscja.deviceapi.exception - package com.rscja.deviceapi.exception
com.rscja.deviceapi.interfaces - package com.rscja.deviceapi.interfaces
com.rscja.scanner - package com.rscja.scanner
com.rscja.scanner.led - package com.rscja.scanner.led
com.rscja.scanner.utility - package com.rscja.scanner.utility
com.rscja.system - package com.rscja.system
com.rscja.utility - package com.rscja.utility
configFDXTag(char[], char[]) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  EM4305 配置成动物标签
  EM4305 configurate animal tag
configFDXTag(char[], char[]) - Method in class com.rscja.deviceapi.RFIDWithLF
  EM4305 配置成动物标签
  EM4305 configurate animal tag
ConfigurationException - Exception in com.rscja.deviceapi.exception
  设备配置异常类
  Device configuration exception type
ConfigurationException() - Constructor for exception com.rscja.deviceapi.exception.ConfigurationException
connect(String, ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.BluetoothReader
connect(String) - Method in class com.rscja.deviceapi.BluetoothReader
connect(String) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  连接蓝牙(Connect Bluetooth)
connect(String, ConnectionStatusCallback<Object>) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  连接蓝牙(Connect Bluetooth)
connect(Context) - Method in class com.rscja.deviceapi.R1HFAndPsamManage
  连接读写器(Connect to the reader)
connect(String, ConnectionStatusCallback<Object>) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
connect(String) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
ConnectionStatus - Enum in com.rscja.deviceapi.interfaces
ConnectionStatusCallback<T> - Interface in com.rscja.deviceapi.interfaces
ConstantUtil - Class in com.idata.scanner.decoder
ConstantUtil() - Constructor for class com.idata.scanner.decoder.ConstantUtil
Consume(float) - Method in class com.rscja.deviceapi.CardWithBYL
  扣费
Consume(float) - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  扣费
convertToRed(String, byte[]) - Method in class com.rscja.utility.FingerprintPictureUtility
cpuCommand(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IHF14443A
  CPU卡发送命令(execute cpu card command)
create() - Method in class com.rscja.deviceapi.entity.HF15693RequestEntity.Builder
CW103_6765 - Static variable in class com.rscja.CWDeviceInfo
CW95_6762 - Static variable in class com.rscja.CWDeviceInfo
CWDeviceInfo - Class in com.rscja

A B C D E F G H I K L M N O P R S T U V W Z