## Uses of Interface
com.rscja.deviceapi.interfaces.ConnectionStatusCallback

- Packages that use ConnectionStatusCallback
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |

- - ### Uses of ConnectionStatusCallback in com.rscja.deviceapi

    Methods in com.rscja.deviceapi with parameters of type ConnectionStatusCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | RFIDWithUHFBLE.`connect(java.lang.String address, ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | BluetoothReader.`connect(java.lang.String address, ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUSB.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUrxUsbToUart.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUrxUart.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置UHF连接状态回调 Setup UHF continuous stauts call-back
    `void` | RFIDWithUHFUrxNetwork.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFUART.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFBLE.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`
    `void` | RFIDWithUHFA8RS232.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> statusCallback)` 设置监听连接状态(Set the listening connection status)
    `void` | RFIDWithUHFA8NetWork.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置监听连接状态(Set the listening connection status)
    `void` | RFIDWithUHFA4RS232.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> statusCallback)` 设置监听连接状态(Set the listening connection status)
    `void` | RFIDWithUHFA4NetWork.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置监听连接状态(Set the listening connection status)
    `void` | BluetoothReader.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)`

  - ### Uses of ConnectionStatusCallback in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces with parameters of type ConnectionStatusCallback
    Modifier and Type | Method and Description
    --- | ---
    `void` | IBluetoothReader.`connect(java.lang.String address, ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 连接蓝牙(Connect Bluetooth)
    `void` | IUHF.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置UHF连接状态回调 Setup UHF continuous stauts call-back
    `void` | IBluetoothReader.`setConnectionStatusCallback(ConnectionStatusCallback<java.lang.Object> btStatusCallback)` 设置蓝牙连接状态的回调(Setup Bluetooth connection status call back)