A B C D E F G H I K L M N O P R S T U V W Z

## I

IBarcode1D - Interface in com.rscja.deviceapi.interfaces
IBarcode2D - Interface in com.rscja.deviceapi.interfaces
IBarcode2DSHardwareInfo - Interface in com.rscja.barcode
IBarcodePhoto - Interface in com.rscja.deviceapi.interfaces
IBarcodePictureCallback - Interface in com.rscja.deviceapi.interfaces
IBarcodeSymbolUtility - Interface in com.rscja.deviceapi.interfaces
IBarcodeUtility - Interface in com.rscja.deviceapi.interfaces
  条码操作类 barcode operate class 注意： Attention: 1、使用前请确认您的机器已安装键盘助手v1.9.0 之后的版本。 1.
IBarcodeVideoCallback - Interface in com.rscja.deviceapi.interfaces
IBluetoothData - Interface in com.rscja.deviceapi.interfaces
IBluetoothData.OnBleDataChangeListener - Interface in com.rscja.deviceapi.interfaces
  接收蓝牙原始数据的接口
  Interface of receiving initial data.
IBluetoothReader - Interface in com.rscja.deviceapi.interfaces
  蓝牙读写器的接口
  Interface of Bluetooth reader.
ICardWithBYL - Interface in com.rscja.deviceapi.interfaces
IFingerprint - Interface in com.rscja.deviceapi.interfaces
IFingerprintSM206B - Interface in com.rscja.deviceapi.interfaces
IFingerprintWithFIPS - Interface in com.rscja.deviceapi.interfaces
IFingerprintWithMorpho - Interface in com.rscja.deviceapi.interfaces
IFingerprintWithTLK1NC - Interface in com.rscja.deviceapi.interfaces
IFingerprintWithZAZ - Interface in com.rscja.deviceapi.interfaces
IGPIStateCallback - Interface in com.rscja.deviceapi.interfaces
IHandheldRFID - Interface in com.rscja.deviceapi.interfaces
IHF14443A - Interface in com.rscja.deviceapi.interfaces
IHF14443B - Interface in com.rscja.deviceapi.interfaces
IHF15693 - Interface in com.rscja.deviceapi.interfaces
IInfrared - Interface in com.rscja.deviceapi.interfaces
ILedLight - Interface in com.rscja.deviceapi.interfaces
IMG_FORMAT_BMP - Static variable in interface com.rscja.deviceapi.interfaces.IBarcodePictureCallback
IMG_FORMAT_JPEG - Static variable in interface com.rscja.deviceapi.interfaces.IBarcodePictureCallback
IMG_FORMAT_TIFF - Static variable in interface com.rscja.deviceapi.interfaces.IBarcodePictureCallback
imgageRawToBimap(byte[]) - Method in class com.rscja.deviceapi.FingerprintSM206B
IModule - Interface in com.rscja.deviceapi.interfaces
IMultipleAntenna - Interface in com.rscja.deviceapi.interfaces
Infrared - Class in com.rscja.deviceapi
  红外模块操作类 Infared module operation type
init(Context) - Method in class com.rscja.deviceapi.BluetoothReader
init() - Method in class com.rscja.deviceapi.CardWithBYL
  初始化RFID和PSAM模块
init() - Method in class com.rscja.deviceapi.Fingerprint
  初始化指纹模块，默认波特率为57600
  Initialize fingerprint module, default baud rate is 57600.
init(int) - Method in class com.rscja.deviceapi.Fingerprint
  初始化指纹模块
  Initialize fingerprint module.
init(Context) - Method in class com.rscja.deviceapi.FingerprintSM206B
  初始化指纹模块
init(Context) - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  初始化指纹模块
  Initialize fingerprint module
init() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
  初始化指纹模块
  Initialize fingerprint module
init() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
  初始化指纹模块
  Initialize fingerprint module
init() - Method in class com.rscja.deviceapi.FingerprintWithTLK1NC
init() - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  初始化指纹模块
  Initialize fingerprint module
init(Context) - Method in interface com.rscja.deviceapi.interfaces.IBluetoothReader
  初始化蓝牙相关的服务(Intialize Bluetooth services)
init() - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
  初始化RFID和PSAM模块
init() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  初始化指纹模块，默认波特率为57600
  Initialize fingerprint module, default baud rate is 57600.
init(int) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  初始化指纹模块
  Initialize fingerprint module.
init(Context) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintSM206B
init(Context) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  初始化指纹模块
  Initialize fingerprint module
init() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
  初始化指纹模块
  Initialize fingerprint module
init() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
  初始化指纹模块
  Initialize fingerprint module
init() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithTLK1NC
init() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  初始化指纹模块
  Initialize fingerprint module
init(int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  初始化模块,模块上电同时打开串口
  Initialize module
init(int, int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  初始化模块,模块上电同时打开串口
init(int, int, int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IModule
  初始化模块 ,模块上电同时打开串口
  Initialize the module
init(int) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
  打开打印机模块
  Switch on printer module
init() - Method in interface com.rscja.deviceapi.interfaces.IPSAM
  初始化PSAM
  Initialize PSAM
init() - Method in interface com.rscja.deviceapi.interfaces.IRFIDBase
  初始化rfid模块
  initialize RFID module
init(boolean) - Method in interface com.rscja.deviceapi.interfaces.IRFIDBase
init() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  初始化RFID低频模块
  Initialize RFID LF module
init(String, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUrxNetwork
init(String, int, boolean) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUrxNetwork
init(UsbDevice, Context) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUrxUsbToUart
init(UsbDevice, Context) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUSB
init(Context) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  初始化UHF模块
  Initiate UHF module
init(int) - Method in class com.rscja.deviceapi.Module
  初始化模块,模块上电同时打开串口
  Initialize module
init(int, int) - Method in class com.rscja.deviceapi.Module
  初始化模块,模块上电同时打开串口
init(int, int, int, int, int) - Method in class com.rscja.deviceapi.Module
  初始化模块 ,模块上电同时打开串口
  Initialize the module
init(int) - Method in class com.rscja.deviceapi.Printer
  打开打印机模块
  Switch on printer module
init() - Method in class com.rscja.deviceapi.PSAM
  初始化PSAM
  Initialize PSAM
init() - Method in class com.rscja.deviceapi.RFIDBase
  初始化rfid模块
  initialize RFID module
init(boolean) - Method in class com.rscja.deviceapi.RFIDBase
init() - Method in class com.rscja.deviceapi.RFIDWithLF
  初始化RFID低频模块
  Initialize RFID LF module
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  连接读写器(Connect reader)
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  连接读写器(Connect reader)
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  连接读写器(Connect reader)
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  连接读写器(Connect reader)
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
init() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  初始化UHF模块,适应所有模块
  Initialize UHF module(Support all modules)
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  初始化UHF模块(仅适用于R2000模块)
  Initialize UHF module(used for R2000 module)
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
  连接UHF模块,在连接uhf模块之前先设置IP、端口 `RFIDWithUHFUrxNetwork.setIPAndPort(String ip, int port)`
  Initiate UHF module `RFIDWithUHFUrxNetwork.setIPAndPort(String ip, int port)`
init(String, int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
  连接uhf模块
  connect UHF module
init(String, int, boolean) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  初始化UHF模块(仅适用于R2000模块)
  Initialize UHF module(used for R2000 module)
init(UsbDevice, Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
  初始化usb相关信息，以及连接usb设备
  initialize USB related information and connect USB device.
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
init(UsbDevice, Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  初始化usb相关信息，以及连接usb设备
  initialize USB related information and connect USB device.
init(Context) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  初始化usb相关信息，以及连接usb设备,默认选择已经发现的usb设备列表的第一个设备
  Initialize USB information and connect USB devices, select USB devices in device list by default.
init(Context) - Method in class com.rscja.scanner.led.ScanLed
  初始化设备资源
  initialize device source
init_R2000() - Method in interface com.rscja.deviceapi.interfaces.IUHFOfAndroidUart
init_R2000() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  初始化UHF模块(仅适用于R2000模块)
  Initialize UHF module(used for R2000 module)
initFW() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
initFW() - Method in class com.rscja.deviceapi.Printer
initPrinterGpio(boolean) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
initPrinterGpio(boolean) - Method in class com.rscja.deviceapi.Printer
initWithNeedleTag() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
  初始化RFID低频模块，针对针管标签
  Initialize RFID LF module, for needle tube tag
initWithNeedleTag() - Method in class com.rscja.deviceapi.RFIDWithLF
  初始化RFID低频模块，针对针管标签
  Initialize RFID LF module, for needle tube tag
inputStatus() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA4
  input status
inputStatus() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFA8
inputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA4
  input status
inputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  获取GPI输入状态
inputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  获取GPIO输入状态
inputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA8
inputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  获取GPI输入状态
inputStatus() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  获取GPIO输入状态
int2Bytes(int) - Static method in class com.rscja.utility.StringUtility
  int转byte数组
Int2bytes(int) - Static method in class com.rscja.utility.StringUtility
int2HexString(int) - Static method in class com.rscja.utility.StringUtility
INT_AIM_128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_AUSPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_AZTEC - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_BOOKLAND - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_BPO - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CANPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CHINAPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODABAR - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODABLOCK - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODABLOCK_A - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODE11 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODE128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODE32 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODE39 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODE39_FULL_ASCII - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODE49 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODE93 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CODE_16K - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_COUPON_CODE - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_CUSTOM_GS1_DATAMATRIX - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_DATAMATRIX - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_DISCRETE_2_OF_5 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_DUTCHPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_EAN13 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_EAN8 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_EAN_128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_GRIDMATRIX - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_GS1_128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_GS1_DATA_MATRIX - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_GS1_DataBar - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_GS1_DataBar_Expanded - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_GS1_DataBar_Limited - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_GS1_QR_CODE - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_HANXIN - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_IATA - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_INFOMAIL - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_INTERLEAVED_2_OF_5 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_ISBT_128 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_ISSN - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_JAPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_KOREAPOST - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_MACRO_PDF - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_MACRO_QR - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_MATRIX25 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_MAXICODE - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_MICRO_QR - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_MICROPDF - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_MSI - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_NEC_2_OF_5 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_PDF417 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_PLANET - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_POSTAL_4I - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_QR - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_TELEPEN - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_TLCODE39 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_TRIOPTIC - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_UPC_D - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_UPC_E1 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_UPCA - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_UPCE0 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_US_POSTALS1 - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
INT_USPS4CB - Static variable in class com.rscja.barcode.BarcodeSymbolUtility
interceptTrimLeft(Context, int) - Method in class com.rscja.barcode.BarcodeUtility
  截取左边字符串数量 Capture left side charactor string amount
interceptTrimLeft(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  截取左边字符串数量 Capture left side charactor string amount
interceptTrimLeft(Context, int) - Method in interface com.rscja.scanner.IScanner
  截取左边字符串
  Capture string on left
interceptTrimLeft(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
interceptTrimRight(Context, int) - Method in class com.rscja.barcode.BarcodeUtility
  截取右边字符串数量 Capture right side charactor string amount
interceptTrimRight(Context, int) - Method in interface com.rscja.deviceapi.interfaces.IBarcodeUtility
  截取右边字符串数量 Capture right side charactor string amount
interceptTrimRight(Context, int) - Method in interface com.rscja.scanner.IScanner
  截取右边字符串
  capture string on right
interceptTrimRight(Context, int) - Method in class com.rscja.scanner.utility.ScannerUtility
ints2HexString(int[], int) - Static method in class com.rscja.utility.StringUtility
inventory() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO15693
  读卡
  read card
inventory() - Method in class com.rscja.deviceapi.RFIDWithISO15693
  读卡
  read card
InventoryModeEntity - Class in com.rscja.deviceapi.entity
InventoryModeEntity.Builder - Class in com.rscja.deviceapi.entity
inventorySingleTag() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
inventorySingleTag() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  单步识别标签
  Identify tag in single mode
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  单次盘点标签(Single Inventory Label)
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  单次盘点标签(Single Inventory Label)
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  单次盘点标签(Single Inventory Label)
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  单次盘点标签(Single Inventory Label)
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  单步识别标签
  Identify tag in single mode
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
inventorySingleTag() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
inventorySingleTagUii() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFRLM
inventorySingleTagUii() - Method in class com.rscja.deviceapi.RFIDWithUHFRLM
ioctl_gpio(int, boolean) - Method in interface com.rscja.deviceapi.interfaces.IModule
ioctl_gpio(int, boolean) - Method in class com.rscja.deviceapi.Module
IPrinter - Interface in com.rscja.deviceapi.interfaces
  打印机操作类
  Printer operation type
IPSAM - Interface in com.rscja.deviceapi.interfaces
IReader - Interface in com.rscja.deviceapi.interfaces
  R2、R5、R6 蓝牙和USB读写器 有些客户只需要我们R6的背夹，不需要uhf模块，所以将R6背夹接口独立出来
IRFIDBase - Interface in com.rscja.deviceapi.interfaces
IRFIDWithISO14443A - Interface in com.rscja.deviceapi.interfaces
IRFIDWithISO14443A4CPU - Interface in com.rscja.deviceapi.interfaces
IRFIDWithISO14443B - Interface in com.rscja.deviceapi.interfaces
IRFIDWithISO15693 - Interface in com.rscja.deviceapi.interfaces
IRFIDWithLF - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFA4 - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFA4NetWork - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFA4RS232 - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFA4Uart - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFA8 - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFA8NetWork - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFA8RS232 - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFA8Uart - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFRLM - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFUrxNetwork - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFUrxUart - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFUrxUsbToUart - Interface in com.rscja.deviceapi.interfaces
IRFIDWithUHFUSB - Interface in com.rscja.deviceapi.interfaces
IScanerLedLight - Interface in com.rscja.deviceapi.interfaces
IScanner - Interface in com.rscja.scanner
isConnected() - Method in class com.rscja.deviceapi.entity.AntennaConnectState
isConnection() - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  检查 Target 和 Host 的连接状态
isConnection() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  检查 Target 和 Host 的连接状态
isDecimal(String) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否是十进制数字
isEmpty(CharSequence) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否为空
isEnable() - Method in class com.rscja.deviceapi.entity.AntennaState
isEnable4G() - Method in interface com.rscja.system.ISystemInterfaces
  判断4G是否启用
isEnableBackKey() - Method in interface com.rscja.system.ISystemInterfaces
  返回按键是否启用
isEnableBeep() - Method in interface com.rscja.deviceapi.interfaces.IUHFURAxExtend
isEnableBeep() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
  是否启用蜂鸣器
isEnableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  是否禁用蜂鸣器
isEnableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  是否禁用蜂鸣器
isEnableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  是否禁用蜂鸣器
isEnableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  是否禁用蜂鸣器
isEnableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
isEnableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  是否启用蜂鸣器
isEnableBeep() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
isEnableBlueth() - Method in interface com.rscja.system.ISystemInterfaces
  判断Blueth是否启用
isEnableCamera() - Method in interface com.rscja.system.ISystemInterfaces
  判断Camera是否启用
isEnableHomeKey() - Method in interface com.rscja.system.ISystemInterfaces
  判断Home按键是否启用
isEnableMenuKey() - Method in interface com.rscja.system.ISystemInterfaces
  判断MenuKey是否启用
isEnableNavigationBar() - Method in interface com.rscja.system.ISystemInterfaces
  判断虚拟导航栏是否启用
isEnableOtg() - Method in interface com.rscja.system.ISystemInterfaces
  判断Otg是否启用
isEnablePanelBar() - Method in interface com.rscja.system.ISystemInterfaces
  判断下拉面板是否启用
isEnableRecentKey() - Method in interface com.rscja.system.ISystemInterfaces
  最近APP使用记录按键是否启用
isEnableScreensho() - Method in interface com.rscja.system.ISystemInterfaces
  判断屏幕截图是否启用
isEnableSystemSettingButton() - Method in interface com.rscja.system.ISystemInterfaces
  判断音量加减界面的设置按钮是否启用
isEnableWifi() - Method in interface com.rscja.system.ISystemInterfaces
  判断wifi是否启用
isHexNumber(String) - Static method in class com.rscja.utility.StringUtility
  Deprecated.
isHexNumberRex(String) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否是十六进制数字，使用正则表达式方式
ISingleAntenna - Interface in com.rscja.deviceapi.interfaces
isIP(String) - Static method in class com.rscja.utility.StringUtility
  验证ip是否合法
isNetworkConnected(Context) - Static method in class com.rscja.utility.NetUtils
  检测网络是否可用
isNum(String) - Static method in class com.rscja.utility.StringUtility
  判断是否为数字
ISO14443A_decrement(int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
ISO14443A_decrement(int, int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
ISO14443A_increment(int, int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  电子钱包充值
  E-wallet charge
ISO14443A_increment(int, int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  电子钱包充值
  E-wallet charge
ISO14443A_initval(int, int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  电子钱包初始化
  E-wallet initialize
ISO14443A_initval(int, int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  电子钱包初始化
  E-wallet initialize
ISO14443A_readval(int) - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithISO14443A
  读取电子钱包余额 传入参数
  read E-wallet balance
ISO14443A_readval(int) - Method in class com.rscja.deviceapi.RFIDWithISO14443A
  读取电子钱包余额 传入参数
  read E-wallet balance
ISO15693Entity - Class in com.rscja.deviceapi.entity
  ISO15693协议数据实体
  ISO15639 protocol data entity
ISO15693Entity(String, String) - Constructor for class com.rscja.deviceapi.entity.ISO15693Entity
  构造函数
  Constructor
ISO15693Entity(String, String, char[]) - Constructor for class com.rscja.deviceapi.entity.ISO15693Entity
  构造函数
  Constructor
ISO15693Entity(String, String, char[], byte[]) - Constructor for class com.rscja.deviceapi.entity.ISO15693Entity
ISO15693Entity(String, String, char[], String, String) - Constructor for class com.rscja.deviceapi.entity.ISO15693Entity
  构造函数
  Constructor
isOctNumber(String) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否是十进制数字
isOctNumberRex(String) - Static method in class com.rscja.utility.StringUtility
  判断字符串是否是十进制数字，使用正则表达式方式
isOpen() - Method in class com.rscja.barcode.BarcodeDecoder
  扫描头是否已经打开
isOpen() - Method in interface com.rscja.deviceapi.interfaces.IZebra2DSoftDecoder
isPowerOn() - Method in class com.rscja.deviceapi.Barcode1D
isPowerOn() - Method in class com.rscja.deviceapi.Barcode2D
isPowerOn() - Method in class com.rscja.deviceapi.CardWithBYL
isPowerOn() - Method in class com.rscja.deviceapi.Fingerprint
isPowerOn() - Method in class com.rscja.deviceapi.FingerprintWithFIPS
isPowerOn() - Method in class com.rscja.deviceapi.FingerprintWithMorpho
isPowerOn() - Method in class com.rscja.deviceapi.FingerprintWithZAZ
isPowerOn() - Method in class com.rscja.deviceapi.Infrared
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IBarcode1D
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IBarcode2D
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.ICardWithBYL
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithFIPS
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithMorpho
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IInfrared
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.ILedLight
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IPrinter
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IPSAM
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IRFIDBase
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithLF
isPowerOn() - Method in interface com.rscja.deviceapi.interfaces.IUHFOfAndroidUart
isPowerOn() - Method in class com.rscja.deviceapi.LedLight
isPowerOn() - Method in class com.rscja.deviceapi.Printer
isPowerOn() - Method in class com.rscja.deviceapi.PSAM
isPowerOn() - Method in class com.rscja.deviceapi.RFIDBase
isPowerOn() - Method in class com.rscja.deviceapi.RFIDWithLF
isPowerOn() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
  判断设备是否上电
  Judge the device is powered on or not.
isReleaseScanKeyOnStopScan() - Method in class com.rscja.deviceapi.entity.ScannerParameterEntity
isStaticIp() - Method in class com.rscja.deviceapi.entity.WifiConfig
isUhfWorking(Context) - Method in interface com.rscja.scanner.IScanner
  UHF 是否正在盘点
  Working status of UHF
isUhfWorking(Context) - Method in class com.rscja.scanner.utility.ScannerUtility
  UHF 是否正在盘点
  Working status of UHF
isWorking() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  uhf 是否正在盘点
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
isWorking() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
ISystemInterfaces - Interface in com.rscja.system
  系统控制接口,目前只支持c66
IUHF - Interface in com.rscja.deviceapi.interfaces
IUHFA4 - Interface in com.rscja.deviceapi.interfaces
IUhfBle - Interface in com.rscja.deviceapi.interfaces
IUHFInventoryCallback - Interface in com.rscja.deviceapi.interfaces
IUHFLocationCallback - Interface in com.rscja.deviceapi.interfaces
IUHFOfAndroidUart - Interface in com.rscja.deviceapi.interfaces
IUHFProtocolParse - Interface in com.rscja.deviceapi.interfaces
IUHFProtocolParseUrx - Interface in com.rscja.deviceapi.interfaces
IUhfReader - Interface in com.rscja.deviceapi.interfaces
  R2、R5、R6 蓝牙和USB读写器包含的uhf特有内容
IUHFURAxExtend - Interface in com.rscja.deviceapi.interfaces
IUHFURx - Interface in com.rscja.deviceapi.interfaces
  UHF UR4特有接口
IUHFUrxAutoInventoryTag - Interface in com.rscja.deviceapi.interfaces
IUpgradeProgress - Interface in com.rscja.deviceapi.interfaces
IURAxOfAndroidUart - Interface in com.rscja.deviceapi.interfaces
IUsbFingerprint - Interface in com.rscja.deviceapi.interfaces
IZebra2DSoftDecoder - Interface in com.rscja.deviceapi.interfaces

A B C D E F G H I K L M N O P R S T U V W Z