A B C D E F G H I K L M N O P R S T U V W Z

## U

UhfBase - Class in com.rscja.deviceapi
UhfBase() - Constructor for class com.rscja.deviceapi.UhfBase
UhfBase.ErrorCode - Class in com.rscja.deviceapi
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  数据块操作
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  数据块操作(Data block operation)
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  数据块操作(Data block operation)
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  数据块操作(Data block operation)
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  数据块操作(Data block operation)
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  数据块操作
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfBlockPermalock(String, int, int, int, String, int, int, int, int, byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
uhfJump2Boot() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  uhf进入boot模式 ，开始升级之前需要调用此函数
  UHF enter boot mode, need to call this formula before upgrade
uhfJump2Boot(int) - Method in interface com.rscja.deviceapi.interfaces.IUHF
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  uhf固件进入boot模式准备升级,调用此函数后需要延时2秒再调用 `RFIDWithUHFA4NetWork.uhfStartUpdate()` (uhf firmware enters boot mode to prepare for upgrade)
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  uhf固件进入boot模式准备升级,调用此函数后需要延时2秒再调用 `RFIDWithUHFA4RS232.uhfStartUpdate()` (uhf firmware enters boot mode to prepare for upgrade)
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  uhf固件进入boot模式准备升级,调用此函数后需要延时2秒再调用 `RFIDWithUHFA8NetWork.uhfStartUpdate()` (uhf firmware enters boot mode to prepare for upgrade)
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  uhf固件进入boot模式准备升级,调用此函数后需要延时2秒再调用 `RFIDWithUHFA8RS232.uhfStartUpdate()` (uhf firmware enters boot mode to prepare for upgrade)
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  uhf进入boot模式 ，开始升级之前需要调用此函数
  UHF enter boot mode, need to call this formula before upgrade
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfJump2Boot() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
uhfJump2Boot(int) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
uhfJump2BootSendData(char) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
uhfJump2BootSTM32() - Method in interface com.rscja.deviceapi.interfaces.IRFIDWithUHFUSB
uhfJump2BootSTM32() - Method in interface com.rscja.deviceapi.interfaces.IUhfBle
uhfJump2BootSTM32() - Method in interface com.rscja.deviceapi.interfaces.IUHFURx
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
  升级STM32主板需要调用此函数进入boot模式
  Upgrade STM32 mainboard that need to call this function to enter boot mode.
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfJump2BootSTM32() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
  升级STM32主板需要调用此函数进入boot模式
  Upgrade STM32 mainboard that need to call this function to enter boot mode.
UHFProtocolParseBase - Class in com.rscja.deviceapi
UHFProtocolParseBase() - Constructor for class com.rscja.deviceapi.UHFProtocolParseBase
uhfStartUpdate() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  开始升级uhf模块
  Start upgrade UHF module
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  开始升级UHF固件,调用此函数后需要延时2秒再调用 `RFIDWithUHFA4NetWork.uhfUpdating(byte[] buff)` (Start to upgrade UHF firmware)
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  开始升级UHF固件,调用此函数后需要延时2秒再调用 `RFIDWithUHFA4RS232.uhfUpdating(byte[] buff)` (Start to upgrade UHF firmware)
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  开始升级UHF固件,调用此函数后需要延时2秒再调用 `RFIDWithUHFA8NetWork.uhfUpdating(byte[] buff)` (Start to upgrade UHF firmware)
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  开始升级UHF固件,调用此函数后需要延时2秒再调用 `RFIDWithUHFA8RS232.uhfUpdating(byte[] buff)` (Start to upgrade UHF firmware)
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  开始升级uhf模块
  Start upgrade UHF module
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfStartUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
uhfStartUpdateSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
uhfStopUpdate() - Method in interface com.rscja.deviceapi.interfaces.IUHF
  停止升级uhf模块，uhf模块升级完成后需要调用此函数
  Stop upgrade UHF module, call this formula after module has been upgraded.
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  停止升级UHF固件(Stop upgrading UHF firmware)
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  停止升级UHF固件(Stop upgrading UHF firmware)
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  停止升级UHF固件(Stop upgrading UHF firmware)
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  停止升级UHF固件(Stop upgrading UHF firmware)
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  停止升级uhf模块，uhf模块升级完成后需要调用此函数
  Stop upgrade UHF module, call this formula after module has been upgraded.
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfStopUpdate() - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
UHFStopUpdateSendData() - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
UHFTAGInfo - Class in com.rscja.deviceapi.entity
UHFTAGInfo() - Constructor for class com.rscja.deviceapi.entity.UHFTAGInfo
uhfUpdating(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHF
  升级uhf模块，发送uhf固件数据
  Upgrade UHF module, send UHF firmware data
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4NetWork
  发送uhf升级包 (Send uhf upgrade package)
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA4RS232
  发送uhf升级包 (Send uhf upgrade package)
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8NetWork
  发送uhf升级包 (Send uhf upgrade package)
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFA8RS232
  发送uhf升级包 (Send uhf upgrade package)
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFBLE
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUART
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxNetwork
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUart
  升级uhf模块，发送uhf固件数据
  Upgrade UHF module, send UHF firmware data
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUrxUsbToUart
uhfUpdating(byte[]) - Method in class com.rscja.deviceapi.RFIDWithUHFUSB
uhfUpdatingSendData(byte[]) - Method in interface com.rscja.deviceapi.interfaces.IUHFProtocolParse
uhfWorkState(boolean) - Method in interface com.rscja.scanner.OnUhfWorkStateListener
  UHF 是否正在盘点
  Working status of UHF
UNKNOWN - Static variable in class com.rscja.barcode.Barcode2DSHardwareInfo
upChar(Fingerprint.BufferEnum) - Method in class com.rscja.deviceapi.Fingerprint
  上传指定缓冲区中的指纹特征数据
  Upload fingerprint feature data of specified buffer zone
upChar(FingerprintWithZAZ.BufferEnum, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  将暂存在RamBuffer中的指纹模板上传到主机
upChar(Fingerprint.BufferEnum) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  上传指定缓冲区中的指纹特征数据
  Upload fingerprint feature data of specified buffer zone
upChar(FingerprintWithZAZ.BufferEnum, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  将暂存在RamBuffer中的指纹模板上传到主机
UPDATE_STM32 - Static variable in interface com.rscja.deviceapi.interfaces.IReader
UPDATE_UHF - Static variable in interface com.rscja.deviceapi.interfaces.IUHF
Upgrade(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPSAM
  固件升级
  Firmware upgrade
Upgrade(int, int, int, byte[]) - Method in class com.rscja.deviceapi.PSAM
  固件升级
  Firmware upgrade
upgradeFont(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
upgradeFont(int, int, int, byte[]) - Method in class com.rscja.deviceapi.Printer
upgradeFW(int, int, int, byte[]) - Method in interface com.rscja.deviceapi.interfaces.IPrinter
upgradeFW(int, int, int, byte[]) - Method in class com.rscja.deviceapi.Printer
upImage(int, String) - Method in class com.rscja.deviceapi.Fingerprint
  上传指纹图像文件
  Upload finerprint image file
upImage(int, String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  上传指纹图像文件
  Upload finerprint image file
upImageData(int, String, int[]) - Method in class com.rscja.deviceapi.FingerprintWithZAZ
  上传指纹图像到外部文件
upImageData(int, String, int[]) - Method in interface com.rscja.deviceapi.interfaces.IFingerprintWithZAZ
  上传指纹图像到外部文件
upImageISO(int, String) - Method in class com.rscja.deviceapi.Fingerprint
  上传指纹ISO图像文件
  Upload fingerprint ISO image file
upImageISO(int, String) - Method in interface com.rscja.deviceapi.interfaces.IFingerprint
  上传指纹ISO图像文件
  Upload fingerprint ISO image file
UsbFingerprint - Class in com.rscja.deviceapi
UsbToFingerprint() - Method in interface com.rscja.deviceapi.interfaces.IUsbFingerprint
UsbToFingerprint() - Method in class com.rscja.deviceapi.UsbFingerprint
UsbToHost() - Method in interface com.rscja.deviceapi.interfaces.IUsbFingerprint
UsbToHost() - Method in class com.rscja.deviceapi.UsbFingerprint

A B C D E F G H I K L M N O P R S T U V W Z