## Uses of Class
com.rscja.deviceapi.RFIDWithISO14443A.KeyType

- Packages that use RFIDWithISO14443A.KeyType
  Package | Description
  --- | ---
  com.rscja.deviceapi |
  com.rscja.deviceapi.interfaces |

- - ### Uses of RFIDWithISO14443A.KeyType in com.rscja.deviceapi

    Methods in com.rscja.deviceapi that return RFIDWithISO14443A.KeyType
    Modifier and Type | Method and Description
    --- | ---
    `static RFIDWithISO14443A.KeyType` | RFIDWithISO14443A.KeyType.`valueOf(java.lang.String name)` Returns the enum constant of this type with the specified name.
    `static RFIDWithISO14443A.KeyType[]` | RFIDWithISO14443A.KeyType.`values()` Returns an array containing the constants of this enum type, in the order they are declared.

    Methods in com.rscja.deviceapi with parameters of type RFIDWithISO14443A.KeyType
    Modifier and Type | Method and Description
    --- | ---
    `SimpleRFIDEntity` | RFIDWithISO14443A.`read(java.lang.String key, RFIDWithISO14443A.KeyType keyType, int sector, int block)` 读卡,此函数包含寻卡和验证密钥步骤 Read card, this formula includes card search and key verfication procedure
    `boolean` | RFIDWithISO14443A.`VerifySector(int sector, java.lang.String key, RFIDWithISO14443A.KeyType keyType)` 验证扇区。S50和S70标签需要使用到此函数。密钥验证通过才可对该扇区进行读写操作。 verificate sector.
    `boolean` | RFIDWithISO14443A.`write(java.lang.String key, RFIDWithISO14443A.KeyType keyType, int sector, int block, java.lang.String hexData)` 写卡，此函数包括寻卡和密钥验证异常 Card writing, this formula includes card searching and key verification err

  - ### Uses of RFIDWithISO14443A.KeyType in com.rscja.deviceapi.interfaces

    Methods in com.rscja.deviceapi.interfaces with parameters of type RFIDWithISO14443A.KeyType
    Modifier and Type | Method and Description
    --- | ---
    `SimpleRFIDEntity` | IRFIDWithISO14443A.`read(java.lang.String key, RFIDWithISO14443A.KeyType keyType, int sector, int block)` 读卡,此函数包含寻卡和验证密钥步骤 Read card, this formula includes card search and key verfication procedure
    `boolean` | IRFIDWithISO14443A.`VerifySector(int sector, java.lang.String key, RFIDWithISO14443A.KeyType keyType)` 验证扇区。S50和S70标签需要使用到此函数。密钥验证通过才可对该扇区进行读写操作。 verificate sector.
    `boolean` | IRFIDWithISO14443A.`write(java.lang.String key, RFIDWithISO14443A.KeyType keyType, int sector, int block, java.lang.String hexData)` 写卡，此函数包括寻卡和密钥验证异常 Card writing, this formula includes card searching and key verification err